<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.8" y2="0" width="0" layer="20"/>
<wire x1="48.8" y1="0" x2="48.8" y2="45.2" width="0" layer="20"/>
<wire x1="48.8" y1="45.2" x2="0" y2="45.2" width="0" layer="20"/>
<wire x1="0" y1="45.2" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="R1206FAB">
</package>
<package name="AYZ0102AGRLC">
</package>
<package name="1X06SMD">
</package>
<package name="EFOBM">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1u"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="IC2" library="fab" package="SOT23" value=""/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="JP2" library="fab" package="2X03SMD" value=""/>
<element name="LED" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="LED-FLAG" library="fab" package="5MM" value="LED5MM"/>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="R2" library="fab" package="R1206FAB" value=""/>
<element name="R3" library="fab" package="R1206FAB" value=""/>
<element name="R4" library="fab" package="R1206FAB" value=""/>
<element name="R5" library="fab" package="R1206FAB" value=""/>
<element name="R6" library="fab" package="R1206FAB" value=""/>
<element name="SW-1" library="fab" package="AYZ0102AGRLC" value="SLIDE-SWITCH"/>
<element name="SW-2" library="fab" package="AYZ0102AGRLC" value="SLIDE-SWITCH"/>
<element name="SW-3" library="fab" package="AYZ0102AGRLC" value="SLIDE-SWITCH"/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$2" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U$3" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="R7" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="U$2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="U$3" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="XTAL-2">
<contactref element="IC1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="SW-3">
<contactref element="IC1" pad="13"/>
<contactref element="SW-3" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="LED" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="SW-1" pad="3"/>
<contactref element="SW-2" pad="3"/>
<contactref element="SW-3" pad="3"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SENSOR">
<contactref element="IC1" pad="12"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SW-2">
<contactref element="IC1" pad="11"/>
<contactref element="SW-2" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SW-1">
<contactref element="IC1" pad="10"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="LED-FLAG">
<contactref element="IC1" pad="6"/>
<contactref element="LED-FLAG" pad="IN"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="U$1" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="RTS">
<contactref element="U$1" pad="6"/>
</signal>
<signal name="XTAL-1">
<contactref element="IC1" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="V-BATTERY">
<contactref element="IC2" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED-FLAG" pad="OUT"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SW-1-AUX">
<contactref element="SW-1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
