<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="7.62" y2="0" width="0.2032" layer="20"/>
<wire x1="7.62" y1="0" x2="7.62" y2="13.97" width="0.2032" layer="20"/>
<wire x1="7.62" y1="13.97" x2="0" y2="13.97" width="0.2032" layer="20"/>
<wire x1="0" y1="13.97" x2="0" y2="0" width="0.2032" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>OUT</text>
<text>QA</text>
<text>v12</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X03">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="QRE1113-1:1">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Testing" package="QRE1113-1:1" value="QRE11131:1"/>
<element name="JP1" library="SparkFun" package="1X03" value=""/>
<element name="JP2" library="SparkFun" package="SFE-LOGO-FLAME" value="LOGO-SFESK"/>
<element name="JP3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$1" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="R2" library="fab" package="R1206FAB" value="10K"/>
<element name="R3" library="fab" package="R1206FAB" value="100"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="OUT">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
