(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 17)
    (no_connects 0)
    (area 168.834999 55.169999 200.735001 85.165001)
    (thickness 1.6)
    (drawings 6)
    (tracks 95)
    (zones 0)
    (modules 7)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 SENSOR)
  (net 4 LED_YELLOW)
  (net 5 LED_RED)
  (net 6 LED_GREEN)
  (net 7 MISO)
  (net 8 SCK)
  (net 9 MOSI)
  (net 10 RESET)
  (net 11 SIGNAL_RED)
  (net 12 SIGNAL_YELLOW)
  (net 13 SIGNAL_GREEN)
  (net 14 XTAL1)
  (net 15 XTAL2)
  (net 16 "Net-(U1-Pad6)")
  (net 17 "Net-(U1-Pad10)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net LED_GREEN)
    (add_net LED_RED)
    (add_net LED_YELLOW)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad6)")
    (add_net RESET)
    (add_net SCK)
    (add_net SENSOR)
    (add_net SIGNAL_GREEN)
    (add_net SIGNAL_RED)
    (add_net SIGNAL_YELLOW)
    (add_net VCC)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (module FabInventory:fab-2X03SMD (layer F.Cu) (tedit 59468717)
    (at 177.8 74.93 270)
    (attr smd)
    (fp_text reference M1 (at 5.715 -3.175 360) (layer F.SilkS))
    (fp_text value ISP (at 0 4.445 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.23 69.85 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 LED_RED))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 SIGNAL_RED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.23 74.93 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 LED_YELLOW))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 SIGNAL_YELLOW))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.23 80.01 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_GREEN))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 SIGNAL_GREEN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Bigshot Custom:fab-1X02SMD" (layer F.Cu) (tedit 59468708)
    (at 196.215 59.055)
    (attr smd)
    (fp_text reference J1 (at 1.905 3.175 180) (layer F.SilkS))
    (fp_text value PWR (at -2.54 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FabInventory:fab-1X06SMD (layer F.Cu) (tedit 594686D1)
    (at 196.215 74.295)
    (attr smd)
    (fp_text reference J2 (at 1.905 8.255 180) (layer F.SilkS))
    (fp_text value EXT_CONN (at -2.54 0 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 SENSOR))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 LED_RED))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 LED_YELLOW))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 LED_GREEN))
  )
  (module "Bigshot Custom:ATTINY84-SSU" (layer F.Cu) (tedit 59468930)
    (at 177.165 62.23 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference U1 (at 5.715 -2.54 360) (layer F.SilkS))
    (fp_text value ATTINY84A (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 XTAL1))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 XTAL2))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 SENSOR))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 SIGNAL_GREEN))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 SIGNAL_YELLOW))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 SIGNAL_RED))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (dimension 29.845 (width 0.3) (layer Dwgs.User)
    (gr_text "29.845 mm" (at 210.265 70.1675 270) (layer Dwgs.User))
    (feature1 (pts (xy 200.66 85.09) (xy 211.615 85.09)))
    (feature2 (pts (xy 200.66 55.245) (xy 211.615 55.245)))
    (crossbar (pts (xy 208.915 55.245) (xy 208.915 85.09)))
    (arrow1a (pts (xy 208.915 85.09) (xy 208.328579 83.963496)))
    (arrow1b (pts (xy 208.915 85.09) (xy 209.501421 83.963496)))
    (arrow2a (pts (xy 208.915 55.245) (xy 208.328579 56.371504)))
    (arrow2b (pts (xy 208.915 55.245) (xy 209.501421 56.371504)))
  )
  (dimension 31.75 (width 0.3) (layer Dwgs.User)
    (gr_text "31.750 mm" (at 184.785 46.275001) (layer Dwgs.User))
    (feature1 (pts (xy 168.91 55.245) (xy 168.91 44.925001)))
    (feature2 (pts (xy 200.66 55.245) (xy 200.66 44.925001)))
    (crossbar (pts (xy 200.66 47.625001) (xy 168.91 47.625001)))
    (arrow1a (pts (xy 168.91 47.625001) (xy 170.036504 47.03858)))
    (arrow1b (pts (xy 168.91 47.625001) (xy 170.036504 48.211422)))
    (arrow2a (pts (xy 200.66 47.625001) (xy 199.533496 47.03858)))
    (arrow2b (pts (xy 200.66 47.625001) (xy 199.533496 48.211422)))
  )
  (gr_line (start 200.66 85.09) (end 200.66 55.245) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 85.09) (end 200.66 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 55.245) (end 168.91 85.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 55.245) (end 168.91 55.245) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.025 84.455) (xy 169.545 84.455) (xy 169.545 66.675) (xy 175.895 66.675) (xy 175.895 55.88)
        (xy 200.025 55.88)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.26 66.04) (xy 169.545 66.04) (xy 169.545 55.88) (xy 175.26 55.88)
      )
    )
  )
)
