(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 23)
    (no_connects 0)
    (area 133.12581 117.272999 179.560286 158.671811)
    (thickness 1.6)
    (drawings 5)
    (tracks 98)
    (zones 0)
    (modules 10)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF1F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ../../../../../../../pngs/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(M1-Pad1)")
  (net 4 "Net-(M2-Pad1)")
  (net 5 "Net-(M2-Pad3)")
  (net 6 "Net-(M3-Pad2)")
  (net 7 TX)
  (net 8 RX)
  (net 9 "Net-(M3-Pad6)")
  (net 10 MISO)
  (net 11 SCK)
  (net 12 MOSI)
  (net 13 RST)
  (net 14 PA0)
  (net 15 PA1)
  (net 16 "Net-(R2-Pad2)")
  (net 17 "Net-(S1-Pad2)")
  (net 18 "Net-(S1-Pad4)")
  (net 19 "Net-(U1-Pad12)")
  (net 20 "Net-(U1-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M2-Pad3)")
    (add_net "Net-(M3-Pad2)")
    (add_net "Net-(M3-Pad6)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net PA0)
    (add_net PA1)
    (add_net RST)
    (add_net RX)
    (add_net SCK)
    (add_net TX)
    (add_net VCC)
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 160.147 125.222)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 1uF (at 2.54 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.39954 0) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 141.732 134.747 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference M1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LEDFAB1206 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(M1-Pad1)"))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 148.59 130.429 270)
    (attr smd)
    (fp_text reference M2 (at 0 0 270) (layer F.SilkS))
    (fp_text value RESONATOR (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(M2-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(M2-Pad3)"))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 168.402 131.318)
    (attr smd)
    (fp_text reference M3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M3-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 TX))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 RX))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M3-Pad6)"))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 158.623 145.415 270)
    (attr smd)
    (fp_text reference M4 (at -0.635 -4.445 270) (layer F.SilkS))
    (fp_text value AVRISPSMD (at 0 4.445 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 RST))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 148.082 134.747 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value 499 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 14 PA0))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(M1-Pad1)"))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 148.082 137.414 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference R2 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value 499 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 15 PA1))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 153.67 125.095 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference R3 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 13 RST))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 142.621 145.796 270)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318 270) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 270) (layer F.SilkS))
    (fp_text user 1 (at -3.683 -2.286 270) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 270) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 270) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(S1-Pad2)"))
    (pad 3 smd rect (at -3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(S1-Pad4)"))
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 156.591 133.096)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -5.375) (layer F.SilkS))
    (fp_text value ATTINY44A-SSU (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(M2-Pad1)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(M2-Pad3)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 RST))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 PA0))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 PA1))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 MOSI))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 RX))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 TX))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 134.62 156.718) (end 134.62 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 156.718) (end 134.62 156.718) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 117.348) (end 177.038 156.718) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 117.348) (end 177.038 117.348) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text Sid+B+L (at 156.21 152.781) (layer F.Cu))
)
