<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<wire x1="91.45151875" y1="57.94891875" x2="51.505890625" y2="57.94891875" width="0.8128" layer="20"/>
<wire x1="51.505890625" y1="57.94891875" x2="51.505890625" y2="20.00328125" width="0.8128" layer="20"/>
<wire x1="51.505890625" y1="20.00328125" x2="91.45151875" y2="20.00328125" width="0.8128" layer="20"/>
<wire x1="91.45151875" y1="20.00328125" x2="91.45151875" y2="57.94891875" width="0.8128" layer="20"/>
</plain>
<libraries>
<library name="fab (1)">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab (1)" package="C1206FAB" value=""/>
<element name="C2" library="fab (1)" package="C1206FAB" value=""/>
<element name="C3" library="fab (1)" package="C1206FAB" value=""/>
<element name="C4" library="fab (1)" package="C1206FAB" value=""/>
<element name="JP1" library="fab (1)" package="2X03SMD" value=""/>
<element name="R1" library="fab (1)" package="R1206FAB" value=""/>
<element name="R2" library="fab (1)" package="R1206FAB" value=""/>
<element name="U$1" library="fab (1)" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="U$2" library="fab (1)" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="U$3" library="fab (1)" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$4" library="fab (1)" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$5" library="fab (1)" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$6" library="fab (1)" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$7" library="fab (1)" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$8" library="fab (1)" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$9" library="fab (1)" package="LED1206FAB" value="LEDFAB1206"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="U$5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="6"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$4" pad="1"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$4" pad="2"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$8" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="2"/>
<contactref element="U$9" pad="2"/>
<contactref element="U$7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$5" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
