<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="2-SMD-5X3MM">
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206" value=""/>
<element name="C2" library="fab" package="C1206" value=""/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="R1" library="fab" package="R1206" value="1K"/>
<element name="R2" library="fab" package="R1206" value="499"/>
<element name="R3" library="fab" package="R1206" value="10K"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="S2" library="fab" package="6MM_SWITCH" value=""/>
<element name="ISP" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="LED1" library="fab" package="LED1206" value="Yellow"/>
<element name="CRYSTAL" library="fab" package="2-SMD-5X3MM" value="20M"/>
<element name="I/O" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="R4" library="fab" package="R1206" value="499"/>
<element name="LED" library="fab" package="LED1206" value="Green"/>
<element name="C4" library="01_SparkFun" package="1206" value="1uF"/>
<element name="C5" library="01_SparkFun" package="1206" value="10uF"/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="ISP" pad="6"/>
<contactref element="LED1" pad="2"/>
<contactref element="S1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="I/O" pad="6"/>
<contactref element="LED" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="ISP" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="S2" pad="3"/>
<contactref element="I/O" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="PB2">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="S1" pad="2"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="XTAL1">
<contactref element="CRYSTAL" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="CRYSTAL" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="10"/>
<contactref element="I/O" pad="4"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="11"/>
<contactref element="I/O" pad="5"/>
</signal>
<signal name="PA1">
<contactref element="IC1" pad="12"/>
<contactref element="I/O" pad="3"/>
</signal>
<signal name="PA0">
<contactref element="IC1" pad="13"/>
<contactref element="I/O" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="PA7">
<contactref element="IC1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
