<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="13.97" y1="33.02" x2="26.67" y2="45.72" width="0.6096" layer="46" curve="-180"/>
<wire x1="26.67" y1="45.72" x2="54.61" y2="39.37" width="0.6096" layer="46" curve="-180"/>
<wire x1="54.61" y1="39.37" x2="54.61" y2="15.24" width="0.6096" layer="46" curve="-180"/>
<wire x1="54.61" y1="15.24" x2="26.67" y2="13.97" width="0.6096" layer="46" curve="-180"/>
<wire x1="26.67" y1="13.97" x2="13.97" y2="33.02" width="0.6096" layer="46" curve="-180"/>
<text>Servo LDR Board</text>
<text>Morining Flowers</text>
<text>May '17</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1-1UF" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="ISP" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="JP1" library="pinhead" package="1X02" value=""/>
<element name="R1-10K" library="fab" package="R1206FAB" value=""/>
<element name="R2-10K" library="fab" package="R1206FAB" value=""/>
<element name="R3-10K" library="fab" package="R1206FAB" value=""/>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="CDS" library="pinhead" package="1X02" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="C1-1UF" pad="1"/>
<contactref element="R2-10K" pad="2"/>
<contactref element="R1-10K" pad="2"/>
<contactref element="ISP" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="ISP" pad="6"/>
<contactref element="U$2" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="C1-1UF" pad="2"/>
<contactref element="CDS" pad="2"/>
</signal>
<signal name="SERVO">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="MOSI-LED">
<contactref element="U$1" pad="5"/>
<contactref element="ISP" pad="4"/>
<contactref element="R3-10K" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="R2-10K" pad="1"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="LDR">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="LDR-MC">
<contactref element="R1-10K" pad="1"/>
<contactref element="CDS" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="1"/>
<contactref element="R3-10K" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
