<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="52.578" y1="-5.842" x2="8.636" y2="-5.842" width="0.3048" layer="20"/>
<wire x1="8.636" y1="-5.842" x2="8.636" y2="66.548" width="0.3048" layer="20"/>
<wire x1="8.636" y1="66.548" x2="52.578" y2="66.548" width="0.3048" layer="20"/>
<wire x1="52.578" y1="66.548" x2="52.578" y2="-5.842" width="0.3048" layer="20"/>
</plain>
<libraries>
<library name="001fab">
<packages>
<package name="C1206FAB">
</package>
<package name="TQFP32-08THIN">
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="OP1206">
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="001fab" package="C1206FAB" value=""/>
<element name="IC1" library="001fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
<element name="R1" library="001fab" package="R1206FAB" value=""/>
<element name="R10" library="001fab" package="R1206FAB" value=""/>
<element name="R11" library="001fab" package="R1206FAB" value=""/>
<element name="R2" library="001fab" package="R1206FAB" value=""/>
<element name="R3" library="001fab" package="R1206FAB" value=""/>
<element name="R4" library="001fab" package="R1206FAB" value=""/>
<element name="R5" library="001fab" package="R1206FAB" value=""/>
<element name="R6" library="001fab" package="R1206FAB" value=""/>
<element name="R7" library="001fab" package="R1206FAB" value=""/>
<element name="R8" library="001fab" package="R1206FAB" value=""/>
<element name="R9" library="001fab" package="R1206FAB" value=""/>
<element name="U$1" library="001fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$10" library="001fab" package="OP1206" value="PHtrans"/>
<element name="U$11" library="001fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$12" library="001fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$13" library="001fab" package="EFOBM" value="RESONATOR"/>
<element name="U$2" library="001fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$3" library="001fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$4" library="001fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$5" library="001fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$6" library="001fab" package="OP1206" value="PHtrans"/>
<element name="U$7" library="001fab" package="OP1206" value="PHtrans"/>
<element name="U$8" library="001fab" package="OP1206" value="PHtrans"/>
<element name="U$9" library="001fab" package="OP1206" value="PHtrans"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="R10" pad="2"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R9" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R8" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="PH5">
<contactref element="IC1" pad="22"/>
<contactref element="R5" pad="2"/>
<contactref element="U$10" pad="COLLECTOR"/>
</signal>
<signal name="PH4">
<contactref element="IC1" pad="23"/>
<contactref element="R4" pad="2"/>
<contactref element="U$9" pad="COLLECTOR"/>
</signal>
<signal name="PH3">
<contactref element="IC1" pad="24"/>
<contactref element="R3" pad="2"/>
<contactref element="U$8" pad="COLLECTOR"/>
</signal>
<signal name="PH2">
<contactref element="IC1" pad="25"/>
<contactref element="R2" pad="2"/>
<contactref element="U$7" pad="COLLECTOR"/>
</signal>
<signal name="PH1">
<contactref element="IC1" pad="26"/>
<contactref element="U$6" pad="COLLECTOR"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="R11" pad="1"/>
<contactref element="U$11" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U$11" pad="6"/>
<contactref element="U$12" pad="1"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="U$10" pad="EMITTER"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$9" pad="EMITTER"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$8" pad="EMITTER"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$7" pad="EMITTER"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$6" pad="EMITTER"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$13" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$11" pad="2"/>
<contactref element="U$12" pad="3"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="18"/>
<contactref element="R6" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$11" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="SCK">
<contactref element="U$11" pad="3"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="U$11" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="TX">
<contactref element="U$12" pad="2"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="RX">
<contactref element="U$12" pad="4"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$4">
<contactref element="U$13" pad="3"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="U$13" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
