<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="USB_MINIB">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C2" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C3" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="C4" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value=""/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="R2" library="fab" package="R1206FAB" value=""/>
<element name="R3" library="fab" package="R1206FAB" value=""/>
<element name="R4" library="fab" package="R1206FAB" value=""/>
<element name="U$1" library="SparkFun-Retired" package="SPARKFUN-DIGITALIC_TQFP44" value="ATMEGA32U4TQFP">
<attribute name="PROD_ID" value="IC-11161"/>
</element>
<element name="U$2" library="fab" package="USB_MINIB" value="USB_MINIB"/>
<element name="U$3" library="fab" package="2-SMD-5X3MM" value="CRYSTAL"/>
<element name="R6" library="fab" package="R1206FAB" value=""/>
<element name="LED1" library="fab" package="P-LCC-4-3" value=""/>
<element name="R5" library="fab" package="R1206FAB" value=""/>
<element name="R7" library="fab" package="R1206FAB" value=""/>
<element name="R8" library="fab" package="R1206FAB" value=""/>
<element name="JP2" library="fab" package="2X03SMD" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="D-"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="D+"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="DM">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="DP">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="23"/>
<contactref element="U$1" pad="35"/>
<contactref element="U$1" pad="43"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="VBUS"/>
<contactref element="U$1" pad="42"/>
<contactref element="U$1" pad="44"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="34"/>
<contactref element="U$1" pad="14"/>
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="2"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="P$1"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="16"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="6"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="6"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="R"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="LED1" pad="B"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="LED1" pad="G"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="U$1" pad="36"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="37"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="38"/>
</signal>
<signal name="SERVO1">
<contactref element="U$1" pad="29"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SERVO2">
<contactref element="U$1" pad="30"/>
<contactref element="JP2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
