<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="0.762" y1="-0.254" x2="24.618" y2="-0.254" width="0" layer="20"/>
<wire x1="24.618" y1="-0.254" x2="24.618" y2="24.816" width="0" layer="20"/>
<wire x1="24.618" y1="24.816" x2="0.762" y2="24.816" width="0" layer="20"/>
<wire x1="0.762" y1="24.816" x2="0.762" y2="-0.254" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="EFOBM">
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="-" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="C1" library="fab" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="CAP-US1206FAB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-DigitalIC" package="SO14" value="ATTINY84">
<attribute name="PROD_ID" value="IC-11285"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$5" library="fab" package="2X03SMD" value="AVRISPSMD"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="14"/>
<contactref element="C1" pad="1"/>
<contactref element="U$5" pad="6"/>
<contactref element="-" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$5" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="U$5" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$5" pad="3"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="RST">
<contactref element="U$5" pad="5"/>
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="-" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="XTAL1">
<contactref element="-" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="C2" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="TX">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="RX">
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="10"/>
<contactref element="S1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
