3d printing
software: pronterface
•	makerbot - more user friendly
•	thing-a-verse

- home - triple home (x,y,z)
lower ^+10 -- raise -10
lower + z -- raise -z
-triple home
lower z
maunally set gome using rings (1,10,100mm)
set screw (focus) > lower z plate, set screw, z home, check height, lower + repeat till satisfactory (can pass piece of paper underneath nozzle with slight resistance)
heat up nozzle (185* > set)
click moniter printer (graphically tracks nozzle temp)
wait for nozzle to heat up
remove excess PLA that oozes out (extrude 65 mm to remove old color)
stabalize rig with index finger
pen with thumb
press in a little bit and remove PLA
insert new PLA bending to the left, stabalize & open, push thru
extrude 65mm
cut 6 inch (hold in back, cut in front)
re-string

SOFTWARE: KISSLICER
open > stl file
blue line = minor error possibility
move & pan like in tinkercad
style > 250 microns > faster good print (100 microns is normal)
support > raft to skirt > support off
material > temp 185
click slice
model + paths, slider to see layers
save as G code
open in pronterface
click print