<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_Arduino-AVR">
<description>&lt;b&gt;Arduino Microcontrollers&lt;/b&gt;
&lt;p&gt;
Atmel ATmega8, ATmega168: 8-bit AVR microcontrollers
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;&lt;i&gt;ATmega8 was used on the original Arduino Serial and USB boards&lt;br&gt;
- 28-pin PDIP (32-lead packages also included)&lt;/i&gt;
&lt;li&gt;ATmega168 for current Arduino Diecimila and NG boards&lt;br&gt;
 - 28-pin PDIP
&lt;li&gt;ATMEGA168 for the Arduino Nano, Mini, LilyPad, Pro and so forth&lt;br&gt;
- 32-lead TQFP and 32-pad QFN/MLF
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;from Rob Faludi: www.faludi.com/projects&lt;/p&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="EFOBM">
</package>
<package name="2X02SMD">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="SMD-RCA-SOCKET">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="01_Arduino-AVR" package="TQFP32-08" value="ATMEGA168-AU"/>
<element name="U$2" library="01_fab" package="EFOBM" value="RESONATOR"/>
<element name="R1" library="01_FAB_Hello" package="1206" value="10K"/>
<element name="R2" library="01_FAB_Hello" package="1206" value="1K"/>
<element name="R3" library="01_FAB_Hello" package="1206" value="499R"/>
<element name="U$3" library="01_FAB_Hello" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$4" library="01_fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="IC2" library="01_fab" package="SOT23" value=""/>
<element name="C1" library="01_ng" package="1206" value="1uF"/>
<element name="U$6" library="01_ng" package="1206" value=""/>
<element name="R6" library="01_ng" package="1206" value=""/>
<element name="S1" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="S2" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="S3" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="S4" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="C2" library="01_FAB_Hello" package="1206" value=""/>
<element name="R4" library="01_FAB_Hello" package="1206" value="3K"/>
<element name="R5" library="01_FAB_Hello" package="1206" value="499R"/>
<element name="U$1" library="01_fab" package="SMD-RCA-SOCKET" value="RCJ-01X-SMT"/>
<element name="U$5" library="01_fab" package="SMD-RCA-SOCKET" value="RCJ-01X-SMT"/>
<element name="R7" library="01_FAB_Hello" package="1206" value="0R"/>
<element name="R8" library="01_FAB_Hello" package="1206" value="0R"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="6"/>
<contactref element="U$4" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$5" pad="GND"/>
<contactref element="U$5" pad="GND2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="15"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="16"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="17"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U$4" pad="3"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="31"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="SIGNAL"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="12"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="2"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="23"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="24"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="25"/>
<contactref element="S3" pad="1"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="26"/>
<contactref element="S4" pad="1"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C2" pad="2"/>
<contactref element="U$5" pad="SIGNAL"/>
</signal>
<signal name="N$15">
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U$3" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="XCLK">
<contactref element="IC1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
