<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.918603125" y1="1.211271875" x2="55.2186" y2="1.51771875" width="0" layer="20"/>
<wire x1="55.2186" y1="1.51771875" x2="55.096" y2="40.9232125" width="0" layer="20"/>
<wire x1="55.096" y1="40.9232125" x2="0.796003125" y2="40.616765625" width="0" layer="20"/>
<wire x1="0.796003125" y1="40.616765625" x2="0.918603125" y2="1.211271875" width="0" layer="20"/>
<text>Pressure Shield</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X04">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="AlexNIMELibrary">
<packages>
<package name="MPXV5010DP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="1X04" value=""/>
<element name="JP3" library="SparkFun" package="1X02_LOCK" value=""/>
<element name="U$1" library="AlexNIMELibrary" package="MPXV5010DP" value="MPXV5010DP"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP3" pad="2"/>
<contactref element="U$1" pad="VS"/>
</signal>
<signal name="GND">
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="A0">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="VOUT"/>
</signal>
<signal name="A1">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="A2">
<contactref element="JP1" pad="2"/>
</signal>
<signal name="A3">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
