<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="17.49643125" x2="0" y2="9.668246875" width="0" layer="20"/>
<wire x1="0" y1="9.668246875" x2="5.668246875" y2="3" width="0" layer="20" curve="90"/>
<wire x1="5.668246875" y1="3" x2="38.724128125" y2="3" width="0" layer="20"/>
<wire x1="38.724128125" y1="3" x2="42.2" y2="7.675871875" width="0" layer="20" curve="90"/>
<wire x1="42.2" y1="7.675871875" x2="42.2" y2="19.83446875" width="0" layer="20"/>
<wire x1="42.2" y1="19.83446875" x2="35.83446875" y2="26.2" width="0" layer="20" curve="90"/>
<wire x1="35.83446875" y1="26.2" x2="7.00356875" y2="26.2" width="0" layer="20"/>
<wire x1="7.00356875" y1="26.2" x2="0" y2="17.49643125" width="0" layer="20" curve="90"/>
<text>TEMP</text>
</plain>
<libraries>
<library name="01_fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="01_fab" package="SOIC8" value="ATTINY45SI"/>
<element name="JP1" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="R1" library="ng" package="1206" value=""/>
<element name="R2" library="ng" package="1206" value=""/>
<element name="R3" library="ng" package="1206" value=""/>
<element name="R4" library="01_ng" package="1206" value=""/>
<element name="R5" library="01_ng" package="1206" value=""/>
<element name="C1" library="01_FAB_Hello" package="1206" value=""/>
<element name="JP2" library="01_FAB_Hello" package="2X03SMD" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$16">
</signal>
<signal name="N$10">
<contactref element="U$1" pad="4"/>
<contactref element="JP2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$2">
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$7">
</signal>
<signal name="N$15">
</signal>
<signal name="N$18">
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
</signals>
</board>
</drawing>
</eagle>
