<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.184" y2="0" width="0" layer="20"/>
<wire x1="48.184" y1="0" x2="48.184" y2="39.36" width="0" layer="20"/>
<wire x1="48.184" y1="39.36" x2="0" y2="39.36" width="0" layer="20"/>
<wire x1="0" y1="39.36" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="01_EasyAccessLib">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel_tiny24-44-84tiny48-88mega48-88-168-328">
<description>Atmel MCUs:

&lt;p&gt;&lt;b&gt;ATmega48/88/168/328&lt;/b&gt; in variants AU, MU, PU
&lt;p&gt;&lt;b&gt;ATtiny24/44/84&lt;/b&gt; in variants SSU, PU, MU
&lt;p&gt;&lt;b&gt;ATtiny48/88&lt;/b&gt; in variants AU, MU, MMU, MMH, PU
&lt;p&gt;&lt;b&gt;AT89C51/52/...&lt;/b&gt;
&lt;p&gt;&lt;b&gt;AT89C1051/2052/4052&lt;/b&gt;

&lt;i&gt;&lt;p&gt;&lt;author&gt;Created by Ing. Miroslav Kovar @ soft&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;b&gt;32A&lt;/b&gt;, 32-lead, 7 x 7 mm Body Size, 1.0 mm Body Thickness, 0.8 mm Lead Pitch, Thin Profile Plastic Quad Flat Package (TQFP)
&lt;p&gt;Atmel</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="20up"/>
<element name="C2" library="fab" package="C1206FAB" value="20up"/>
<element name="C3" library="fab" package="C1206FAB" value="0.1up"/>
<element name="C4" library="fab" package="C1206FAB" value="1up"/>
<element name="FTDI" library="01_EasyAccessLib" package="1X06" value=""/>
<element name="IC1" library="atmel_tiny24-44-84tiny48-88mega48-88-168-328" package="TQFP32-08" value=""/>
<element name="ISP" library="fab" package="2X03SMD" value=""/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="10K"/>
<element name="R3" library="fab" package="R1206FAB" value="10K"/>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49US" value=""/>
<element name="R2" library="fab" package="R1206FAB" value="0"/>
<element name="R4" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="FTDI" pad="1"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="4"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="6"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="3"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="C1" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="10"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="FTDI" pad="6"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="FTDI" pad="3"/>
<contactref element="ISP" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="CTS">
<contactref element="IC1" pad="32"/>
<contactref element="FTDI" pad="2"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="30"/>
<contactref element="FTDI" pad="4"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="31"/>
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="ISP" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
