<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="2.4638" y1="1.3716" x2="49.962" y2="1.397" width="0" layer="20"/>
<wire x1="49.962" y1="1.397" x2="49.9874" y2="43.297" width="0" layer="20"/>
<wire x1="49.9874" y1="43.297" x2="2.5146" y2="43.3224" width="0" layer="20"/>
<wire x1="2.5146" y1="43.3224" x2="2.4638" y2="1.3716" width="0" layer="20"/>
</plain>
<libraries>
<library name="ng">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="2X03SMD">
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM-NS">
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="14PA">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-alps">
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="ng" package="1206" value=".1uf"/>
<element name="IC1" library="atmega8" package="TQFP32-08" value="ATMEGA48/88/168-AU"/>
<element name="LED" library="ng" package="1206" value=""/>
<element name="R2" library="ng" package="1206" value="499"/>
<element name="U$2" library="fab" package="EFOBM" value="RESONATOREFOB">
<attribute name="VARIANT" value=""/>
</element>
<element name="U$1" library="01_FAB_Hello" package="2X03SMD" value="AVRISPSMD"/>
<element name="C5" library="ng" package="1206" value="10uf"/>
<element name="SV3" library="con-lstb" package="MA06-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="ng" package="1206" value="1k"/>
<element name="R3" library="ng" package="1206" value="470"/>
<element name="R4" library="ng" package="1206" value="1k"/>
<element name="LED1" library="01_fab" package="P-LCC-4-3" value=""/>
<element name="SG1" library="01_SparkFun" package="BUZZER-12MM-NS" value="BUZZERNS"/>
<element name="SL1" library="con-amp-quick" package="14PA" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R6" library="ng" package="1206" value="10k"/>
<element name="R7" library="ng" package="1206" value="1k"/>
<element name="R8" library="ng" package="1206" value="0"/>
<element name="SW1" library="switch-alps" package="ALPS_EC12E_SW" value="EC12E_SW">
<attribute name="OC_NEWARK" value="74M1068"/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1520813"/>
</element>
<element name="C1" library="01_FAB_Hello" package="1206" value=""/>
<element name="C2" library="01_FAB_Hello" package="1206" value=""/>
<element name="R9" library="ng" package="1206" value="10k"/>
<element name="R10" library="ng" package="1206" value="10k"/>
<element name="R11" library="ng" package="1206" value="10k"/>
<element name="R12" library="ng" package="1206" value="10k"/>
<element name="R13" library="ng" package="1206" value="10k"/>
<element name="S1" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="R14" library="ng" package="1206" value="10k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="LED" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="C5" pad="1"/>
<contactref element="SV3" pad="6"/>
<contactref element="SG1" pad="-"/>
<contactref element="SL1" pad="14"/>
<contactref element="SL1" pad="10"/>
<contactref element="R6" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="SW1" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="SW1" pad="E"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="29"/>
<contactref element="U$1" pad="5"/>
<contactref element="SV3" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="R14" pad="1"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="17"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="R2" pad="2"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="7"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="5V">
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="SV3" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="6"/>
<contactref element="LED1" pad="A"/>
<contactref element="SL1" pad="13"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="12V">
<contactref element="SV3" pad="4"/>
</signal>
<signal name="PD0">
<contactref element="IC1" pad="30"/>
</signal>
<signal name="PD1">
<contactref element="IC1" pad="31"/>
<contactref element="SG1" pad="+"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="G"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="B"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="R"/>
</signal>
<signal name="PC0">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="ADC6">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$6">
<contactref element="SL1" pad="12"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="PD6">
<contactref element="SL1" pad="9"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="PB2">
<contactref element="SL1" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="PB1">
<contactref element="SL1" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PB0">
<contactref element="SL1" pad="3"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="PD5">
<contactref element="SL1" pad="11"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="PD7">
<contactref element="SL1" pad="4"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="R11" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="SW1" pad="B"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R12" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="SW1" pad="A"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="PC2">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="INT0">
<contactref element="IC1" pad="32"/>
<contactref element="R10" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="INT1">
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="SWBUTTON">
<contactref element="IC1" pad="2"/>
<contactref element="SW1" pad="D"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="PC1">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
