<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="1.27" x2="17.45" y2="1.27" width="0" layer="20"/>
<wire x1="17.45" y1="1.27" x2="17.45" y2="30.47" width="0" layer="20"/>
<wire x1="17.45" y1="30.47" x2="1.27" y2="30.47" width="0" layer="20"/>
<wire x1="1.27" y1="30.47" x2="1.27" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="R1206FAB">
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="00fab" package="R1206FAB" value=""/>
<element name="U$1" library="00fab" package="5MM" value="LED5MM"/>
<element name="U$2" library="00fab" package="2X03" value="AVRISP"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="IN"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="OUT"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
