<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="18.42203125" y1="6.697609375" x2="13.21503125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="6.697609375" x2="13.21503125" y2="17.841859375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="17.841859375" x2="10.04003125" y2="17.841859375" width="0.001" layer="20"/>
<wire x1="10.04003125" y1="17.841859375" x2="10.04003125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="10.04003125" y1="6.697609375" x2="1.97553125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="1.97553125" y1="6.697609375" x2="1.97553125" y2="25.874609375" width="0.001" layer="20"/>
<wire x1="1.97553125" y1="25.874609375" x2="7.62703125" y2="25.874609375" width="0.001" layer="20"/>
<wire x1="7.62703125" y1="25.874609375" x2="7.62703125" y2="31.176859375" width="0.001" layer="20"/>
<wire x1="7.62703125" y1="31.176859375" x2="13.21503125" y2="31.176859375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="31.176859375" x2="13.21503125" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="36.733109375" x2="18.42203125" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="18.42203125" y1="36.733109375" x2="18.42203125" y2="39.558859375" width="0.001" layer="20"/>
<wire x1="18.42203125" y1="39.558859375" x2="13.21503125" y2="39.558859375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="39.558859375" x2="13.21503125" y2="45.337359375" width="0.001" layer="20"/>
<wire x1="13.21503125" y1="45.337359375" x2="20.86678125" y2="45.337359375" width="0.001" layer="20"/>
<wire x1="20.86678125" y1="45.337359375" x2="20.86678125" y2="42.321109375" width="0.001" layer="20"/>
<wire x1="20.86678125" y1="42.321109375" x2="26.45478125" y2="42.321109375" width="0.001" layer="20"/>
<wire x1="26.45478125" y1="42.321109375" x2="26.45478125" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="26.45478125" y1="36.733109375" x2="40.45653125" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="40.45653125" y1="36.733109375" x2="40.45653125" y2="42.321109375" width="0.001" layer="20"/>
<wire x1="40.45653125" y1="42.321109375" x2="46.04453125" y2="42.321109375" width="0.001" layer="20"/>
<wire x1="46.04453125" y1="42.321109375" x2="46.04453125" y2="45.337359375" width="0.001" layer="20"/>
<wire x1="46.04453125" y1="45.337359375" x2="53.75976875" y2="45.337359375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="45.337359375" x2="53.75976875" y2="39.558859375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="39.558859375" x2="48.52103125" y2="39.558859375" width="0.001" layer="20"/>
<wire x1="48.52103125" y1="39.558859375" x2="48.52103125" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="48.52103125" y1="36.733109375" x2="53.75976875" y2="36.733109375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="36.733109375" x2="53.75976875" y2="31.176859375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="31.176859375" x2="59.31603125" y2="31.176859375" width="0.001" layer="20"/>
<wire x1="59.31603125" y1="31.176859375" x2="59.31603125" y2="25.874609375" width="0.001" layer="20"/>
<wire x1="59.31603125" y1="25.874609375" x2="64.93578125" y2="25.874609375" width="0.001" layer="20"/>
<wire x1="64.93578125" y1="25.874609375" x2="64.93578125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="64.93578125" y1="6.697609375" x2="56.90303125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="56.90303125" y1="6.697609375" x2="56.90303125" y2="17.841859375" width="0.001" layer="20"/>
<wire x1="56.90303125" y1="17.841859375" x2="53.75976875" y2="17.841859375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="17.841859375" x2="53.75976875" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="53.75976875" y1="6.697609375" x2="48.52103125" y2="6.697609375" width="0.001" layer="20"/>
<wire x1="48.52103125" y1="6.697609375" x2="48.52103125" y2="1.427109375" width="0.001" layer="20"/>
<wire x1="48.52103125" y1="1.427109375" x2="34.86853125" y2="1.427109375" width="0.001" layer="20"/>
<wire x1="34.86853125" y1="1.427109375" x2="34.86853125" y2="9.428109375" width="0.001" layer="20"/>
<wire x1="34.86853125" y1="9.428109375" x2="46.04453125" y2="9.428109375" width="0.001" layer="20"/>
<wire x1="46.04453125" y1="9.428109375" x2="46.04453125" y2="12.285609375" width="0.001" layer="20"/>
<wire x1="46.04453125" y1="12.285609375" x2="20.86678125" y2="12.285609375" width="0.001" layer="20"/>
<wire x1="20.86678125" y1="12.285609375" x2="20.86678125" y2="9.428109375" width="0.001" layer="20"/>
<wire x1="20.86678125" y1="9.428109375" x2="32.10628125" y2="9.428109375" width="0.001" layer="20"/>
<wire x1="32.10628125" y1="9.428109375" x2="32.10628125" y2="1.427109375" width="0.001" layer="20"/>
<wire x1="32.10628125" y1="1.427109375" x2="18.42203125" y2="1.427109375" width="0.001" layer="20"/>
<wire x1="18.42203125" y1="1.427109375" x2="18.42203125" y2="6.697609375" width="0.001" layer="20"/>
</plain>
<libraries>
<library name="fab (1)">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="SPDTSWITCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab (1)" package="C1206FAB" value="1uF"/>
<element name="JP1" library="fab (1)" package="2X03SMD" value=""/>
<element name="R1" library="fab (1)" package="R1206" value="1K"/>
<element name="R2" library="fab (1)" package="R1206" value="10K"/>
<element name="U$1" library="fab (1)" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab (1)" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$3" library="fab (1)" package="LED1206FAB" value="LED"/>
<element name="U$4" library="fab" package="SPDTSWITCH" value="SPDTSWITCH"/>
<element name="U$5" library="fab" package="SPDTSWITCH" value="SPDTSWITCH"/>
<element name="R3" library="fab (1)" package="R1206" value="0"/>
<element name="R4" library="fab (1)" package="R1206" value="0"/>
<element name="R5" library="fab (1)" package="R1206" value="0"/>
<element name="R6" library="fab (1)" package="R1206" value="0"/>
<element name="R7" library="fab (1)" package="R1206" value="0"/>
<element name="R8" library="fab (1)" package="R1206" value="0"/>
<element name="R9" library="fab (1)" package="R1206" value="0"/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="JP1" pad="5"/>
<contactref element="U$2" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$4" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$5" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
