(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 48)
    (no_connects 7)
    (area 135.905999 105.933211 194.998286 148.828001)
    (thickness 1.6)
    (drawings 4)
    (tracks 169)
    (zones 0)
    (modules 20)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.45)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3)
    (segment_width 0.2)
    (edge_width 2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.54 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(D1-Pad2)")
  (net 4 LED1_out)
  (net 5 BTN1)
  (net 6 MOSI)
  (net 7 MISO)
  (net 8 SCK)
  (net 9 "Net-(IC1-Pad12)")
  (net 10 "Net-(IC1-Pad13)")
  (net 11 "Net-(C2-Pad1)")
  (net 12 "Net-(C3-Pad2)")
  (net 13 Light)
  (net 14 RST)
  (net 15 HALL)
  (net 16 "Net-(M2-Pad2)")
  (net 17 "Net-(M2-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.45)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BTN1)
    (add_net GND)
    (add_net HALL)
    (add_net LED1_out)
    (add_net Light)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M2-Pad6)")
    (add_net RST)
    (add_net SCK)
    (add_net VCC)
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 169.799 123.444 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 360) (layer B.SilkS))
    (fp_text value ATTINY44-SSU (at 1.27 0.0635 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 RST))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 LED1_out))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 BTN1))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 HALL))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 Light))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 170.434 139.065 180)
    (attr smd)
    (fp_text reference M1 (at -0.635 -4.445 180) (layer B.SilkS))
    (fp_text value AVRISPSMD (at 0 4.445 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 MISO))
    (pad 2 smd rect (at 2.91846 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -2.54 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 4 smd rect (at 2.91846 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 5 smd rect (at -2.54 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 RST))
    (pad 6 smd rect (at 2.91846 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 168.53154 113.03 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at 1.905 -1.905 180) (layer B.SilkS))
    (fp_text value 1u (at 2.92354 2.286 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 150.368 117.856)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D1 (at 1.905 -1.905) (layer B.SilkS))
    (fp_text value LED (at 2.54 1.905) (layer B.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 168.55186 116.586)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.905) (layer B.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer B.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 RST))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 155.448 117.856 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at 1.905 -1.905 180) (layer B.SilkS))
    (fp_text value RES-US1206 (at 2.54 1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 LED1_out))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 153.162 122.682)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318) (layer B.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 BTN1))
    (pad 2 smd rect (at 3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 BTN1))
    (pad 3 smd rect (at -3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 143.764 114.046 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 162.814 112.014 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 5418A1CA)
    (at 183.515 132.321 90)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R3 (at 0 -3.1 90) (layer F.SilkS))
    (fp_text value Photores (at 0 3.1 90) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 90) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 3.95 0 90) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 13 Light))
    (model Resistors_SMD.3dshapes/R_2512_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 183.595 132.461 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 Light))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 0)
    (at 153.162 113.03)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference X1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value CRYSTAL_SMD (at 2.54 5.08) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 4.84886 0) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C3-Pad2)"))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 571CFBE7)
    (at 183.515 118.872)
    (attr smd)
    (fp_text reference M2 (at -2.54 0 90) (layer B.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 0 -10.16) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(M2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad13)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M2-Pad6)"))
  )
  (module fablab-inventory:Pin_Header_Angled_SMD_1X04 (layer F.Cu) (tedit 56DAB1D1)
    (at 153.162 138.047 180)
    (fp_text reference P1 (at -6.35 3.81 270) (layer F.SilkS))
    (fp_text value Header_angled_SMT_1X04 (at 0 7.62 180) (layer F.Fab))
    (pad 1 smd rect (at -3.81 5.205 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 2 smd oval (at -1.27 5.205 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 3 smd oval (at 1.27 5.205 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd oval (at 3.81 5.205 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 177.8 129.54 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference IC2 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value A1301KLHLT-T (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 HALL))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 173.355 115.062 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 182.608786 141.333786 135)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -2.3 135) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 135) (layer F.Fab))
    (pad 1 smd rect (at -2 0 135) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 2 0 135) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 162.211 140.589)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 162.179 137.668)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 177.419 113.03 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.906 147.828) (end 136.906 106.933212) (layer Edge.Cuts) (width 2))
  (gr_line (start 190.627 147.828) (end 136.906 147.828) (layer Edge.Cuts) (width 2))
  (gr_line (start 190.627 106.933212) (end 190.627 147.828) (layer Edge.Cuts) (width 2))
  (gr_line (start 136.906 106.934) (end 190.627 106.934) (layer Edge.Cuts) (width 2))
)
