<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2X03SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
<library name="ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="A3216-18">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FTDI" library="SparkFun-Connectors" package="1X06-SMD" value="">
<attribute name="PROD_ID" value="CONN-08971"/>
</element>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="BUS" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="C1" library="ng" package="A3216-18" value=""/>
<element name="R3" library="ng" package="1206" value="10k"/>
<element name="POT" library="SparkFun-Connectors" package="1X06-SMD" value="RA 6Pin SMD">
<attribute name="PROD_ID" value="CONN-08971"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="FTDI" pad="6"/>
<contactref element="JP1" pad="1"/>
<contactref element="BUS" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="-"/>
<contactref element="POT" pad="2"/>
</signal>
<signal name="CTS">
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="FTDI" pad="4"/>
<contactref element="JP1" pad="5"/>
<contactref element="BUS" pad="4"/>
<contactref element="C1" pad="+"/>
<contactref element="U$1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="POT" pad="6"/>
</signal>
<signal name="TX">
<contactref element="FTDI" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="BUS" pad="3"/>
</signal>
<signal name="RX">
<contactref element="FTDI" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="BUS" pad="1"/>
</signal>
<signal name="RTS">
<contactref element="FTDI" pad="1"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
</signal>
<signal name="MOSI/SDA">
<contactref element="U$1" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SCK/SCL">
<contactref element="U$1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO/POT">
<contactref element="U$1" pad="6"/>
<contactref element="POT" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
