(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 24)
    (no_connects 0)
    (area 175.438999 75.198689 210.623286 110.819001)
    (thickness 1.6)
    (drawings 6)
    (tracks 131)
    (zones 0)
    (modules 11)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x01000_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 /PB3)
  (net 7 "Net-(IC1-Pad5)")
  (net 8 "Net-(IC1-Pad6)")
  (net 9 /PA6)
  (net 10 /PA5)
  (net 11 /PA4)
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 /PA1)
  (net 15 /PA0)
  (net 16 "Net-(J2-Pad2)")
  (net 17 "Net-(J2-Pad6)")
  (net 18 "Net-(R2-Pad1)")
  (net 19 "Net-(S1-Pad1)")
  (net 20 "Net-(S1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PB3)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad3)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 56FA7FB8)
    (at 182.118 106.426)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 187.96 85.09 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 15pF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 191.262 85.09 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 15pF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 179.832 96.52 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2 270) (layer F.SilkS))
    (fp_text value LED (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 191.516 94.742 180)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 270) (layer B.SilkS))
    (fp_text value ATTINY44A-SS (at 1.27 0.0635 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.54 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -1.27 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 0 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB3))
    (pad 5 smd rect (at 1.27 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 2.54 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 3.81 2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 /PA6))
    (pad 8 smd rect (at 3.81 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 /PA5))
    (pad 9 smd rect (at 2.54 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 /PA4))
    (pad 10 smd rect (at 1.27 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA1))
    (pad 13 smd rect (at -2.54 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 /PA0))
    (pad 14 smd rect (at -3.81 -2.6035 180) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 191.516 104.648)
    (attr smd)
    (fp_text reference J1 (at -0.635 -4.445) (layer B.SilkS))
    (fp_text value AVRISP (at 0 4.445) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 /PA5))
    (pad 2 smd rect (at 2.91846 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /PA4))
    (pad 4 smd rect (at 2.91846 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 /PA6))
    (pad 5 smd rect (at -2.54 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB3))
    (pad 6 smd rect (at 2.91846 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 199.39 95.504 180)
    (attr smd)
    (fp_text reference J2 (at -2.54 0 270) (layer B.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.81 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 /PA0))
    (pad 5 smd rect (at 0 3.81 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA1))
    (pad 6 smd rect (at 0 6.35 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad6)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 56FA7FAC)
    (at 182.118 102.87 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 184.404 96.52 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 182.118 86.614 270)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318 270) (layer B.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 270) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286 270) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 270) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 270) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(S1-Pad1)"))
    (pad 2 smd rect (at 3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(S1-Pad3)"))
    (pad 4 smd rect (at 3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module fab:fab-2-SMD-5X3MM (layer F.Cu) (tedit 200000)
    (at 195.072 85.09 90)
    (attr smd)
    (fp_text reference XTAL1 (at 0.635 -3.175 90) (layer B.SilkS))
    (fp_text value 20M (at 1.27 3.175 90) (layer B.SilkS))
    (pad P$1 smd rect (at -1.99898 0 90) (size 1.99898 2.39776) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad P$2 smd rect (at 1.99898 0 90) (size 1.99898 2.39776) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (gr_line (start 175.514 80.518) (end 175.514 80.772) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.454 80.518) (end 175.514 80.518) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.454 110.744) (end 203.454 80.518) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.692 110.744) (end 203.454 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 110.744) (end 202.692 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 80.772) (end 175.514 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.454 110.744) (xy 175.514 110.744) (xy 175.514 80.518) (xy 203.454 80.518) (xy 203.454 110.744)
      )
    )
  )
)
