<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="29.21" y1="11.43" x2="69.52" y2="11.43" width="0" layer="20"/>
<wire x1="69.52" y1="11.43" x2="69.52" y2="29.2" width="0" layer="20"/>
<wire x1="69.52" y1="29.2" x2="29.21" y2="29.2" width="0" layer="20"/>
<wire x1="29.21" y1="29.2" x2="29.21" y2="11.43" width="0" layer="20"/>
<text>G00 X6000</text>
<hole x="63.5" y="25.4" drill="1"/>
<hole x="63.5" y="22.86" drill="1"/>
<hole x="63.5" y="20.32" drill="1"/>
<hole x="63.5" y="17.78" drill="1"/>
<hole x="63.5" y="15.24" drill="1"/>
<hole x="63.5" y="12.7" drill="1"/>
</plain>
<libraries>
<library name="01_fab1">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="06P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_fab1" package="C1206FAB" value="1 mf"/>
<element name="R1" library="01_fab1" package="R1206FAB" value="10 k"/>
<element name="R2" library="01_fab1" package="R1206FAB" value="1 K"/>
<element name="S1" library="01_fab1" package="6MM_SWITCH" value=""/>
<element name="SL1" library="con-amp-quick" package="06P" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="U$1" library="01_fab1" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="01_fab1" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$3" library="01_fab1" package="LED1206FAB" value="LEDFAB1206"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="2"/>
<contactref element="SL1" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="SL1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RX">
<contactref element="SL1" pad="5"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="R2">
<contactref element="U$1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
