(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu14.04.1)
  (general
    (links 22)
    (no_connects 0)
    (area 142.824999 45.669999 186.740001 88.315001)
    (thickness 1.6)
    (drawings 4)
    (tracks 98)
    (zones 0)
    (modules 9)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 XTAL1)
  (net 5 XTAL2)
  (net 6 RESET)
  (net 7 LED)
  (net 8 SWITCH)
  (net 9 MOSI)
  (net 10 MISO)
  (net 11 SCK)
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 RX)
  (net 15 TX)
  (net 16 "Net-(J2-Pad2)")
  (net 17 "Net-(J2-Pad6)")
  (net 18 "Net-(SW1-Pad2)")
  (net 19 "Net-(SW1-Pad4)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net LED)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad4)")
    (add_net RESET)
    (add_net RX)
    (add_net SCK)
    (add_net SWITCH)
    (add_net TX)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (module FabInventory:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 170.18 53.975 270)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 1.778 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FabInventory:fab-LED1206FAB (layer F.Cu) (tedit 200000)
    (at 150.495 65.405)
    (descr "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (tags "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (attr smd)
    (fp_text reference D1 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value LED (at 1.27 1.778) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module FabInventory:fab-SOIC14 (layer F.Cu) (tedit 58BF2F6E)
    (at 167.64 62.23 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 360) (layer F.SilkS))
    (fp_text value ATTINY44-SSU (at 1.27 0.0635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 RESET))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 LED))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 SWITCH))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 RX))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 TX))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FabInventory:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 171.45 77.47 270)
    (attr smd)
    (fp_text reference J1 (at -0.635 -4.445 270) (layer F.SilkS))
    (fp_text value ISP (at 0 4.445 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 RESET))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module FabInventory:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 177.165 62.23)
    (attr smd)
    (fp_text reference J2 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 TX))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 RX))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad6)"))
  )
  (module FabInventory:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 165.1 53.975 270)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778 270) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.778 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 6 RESET))
  )
  (module FabInventory:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 156.845 65.405 180)
    (attr smd)
    (fp_text reference R2 (at 0.762 -1.778 180) (layer F.SilkS))
    (fp_text value 160 (at 1.27 1.778 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 7 LED))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
  )
  (module FabInventory:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 155.575 76.835 270)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference SW1 (at 0.127 -4.318 270) (layer F.SilkS))
    (fp_text value 6MM_SWITCH (at 0.762 4.445 270) (layer F.SilkS))
    (fp_text user 1 (at -3.683 -2.286 270) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 270) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 270) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 SWITCH))
    (pad 2 smd rect (at 3.302 -2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(SW1-Pad2)"))
    (pad 3 smd rect (at -3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 3.302 2.286 270) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(SW1-Pad4)"))
  )
  (module FabInventory:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 158.75 60.325 270)
    (attr smd)
    (fp_text reference XTAL1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 20MHz (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 XTAL1))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 XTAL2))
  )
  (gr_line (start 142.875 88.265) (end 142.875 45.72) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.69 88.265) (end 142.875 88.265) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.69 45.72) (end 186.69 88.265) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.875 45.72) (end 186.69 45.72) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 87.63) (xy 143.51 87.63) (xy 143.51 46.355) (xy 186.055 46.355)
      )
    )
  )
)
