<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0.127" y1="12.446" x2="73.547" y2="12.446" width="0" layer="20"/>
<wire x1="73.547" y1="12.446" x2="73.547" y2="50.042" width="0" layer="20"/>
<wire x1="73.547" y1="50.042" x2="0.127" y2="50.042" width="0" layer="20"/>
<wire x1="0.127" y1="50.042" x2="0.127" y2="12.446" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="2X02SMD">
</package>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SE11">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.1 mm</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="10uF"/>
<element name="C2" library="fab" package="C1206FAB" value="1uF"/>
<element name="C3" library="fab" package="C1206FAB" value="1uF"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="LED1" library="fab" package="LED1206FAB" value="Red"/>
<element name="R5" library="fab" package="R1206FAB" value="1k"/>
<element name="R6" library="fab" package="R1206FAB" value="500 ohm"/>
<element name="LED3" library="fab" package="LED1206FAB" value="network notice led"/>
<element name="SERVO_CONNECTOR1" library="fab" package="2X03SMD" value="2x3 header"/>
<element name="HALL_CONNECTOR1" library="fab" package="2X02SMD" value="2x2 header"/>
<element name="5V_REGU1" library="fab" package="SOT23" value="5v regu"/>
<element name="C8" library="fab" package="C1206FAB" value="0.1uF"/>
<element name="C9" library="fab" package="C1206FAB" value="0.1uF"/>
<element name="POWER_IN1" library="fab" package="2X02SMD" value="2x2 header"/>
<element name="D2" library="fab" package="MINI-SMA" value="Diodi schottky"/>
<element name="47UF1" library="solpad" package="SE11" value="enable_1"/>
<element name="47UF3" library="solpad" package="SE11" value="enable_1"/>
<element name="ISP1" library="fab" package="2X03SMD" value="2x3 header"/>
<element name="NETWORK1" library="fab" package="2X02SMD" value="2x2 header"/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="R2" library="fab" package="R1206FAB" value="0ohm"/>
<element name="R3" library="fab" package="R1206FAB" value="0ohm"/>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="C4" library="fab" package="C1206FAB" value="10uF"/>
<element name="C5" library="fab" package="C1206FAB" value="10uF"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
<contactref element="LED1" pad="2"/>
<contactref element="HALL_CONNECTOR1" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="5V_REGU1" pad="1"/>
<contactref element="D2" pad="ANODE"/>
<contactref element="ISP1" pad="2"/>
<contactref element="HALL_CONNECTOR1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="SERVO_CONNECTOR1" pad="1"/>
<contactref element="SERVO_CONNECTOR1" pad="2"/>
<contactref element="HALL_CONNECTOR1" pad="3"/>
<contactref element="5V_REGU1" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="POWER_IN1" pad="1"/>
<contactref element="47UF3" pad="MP"/>
<contactref element="ISP1" pad="6"/>
<contactref element="NETWORK1" pad="4"/>
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="ISP1" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="V_IN">
<contactref element="C8" pad="1"/>
<contactref element="5V_REGU1" pad="2"/>
<contactref element="POWER_IN1" pad="2"/>
<contactref element="47UF1" pad="MP"/>
<contactref element="D2" pad="KATHODE"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="RX">
<contactref element="NETWORK1" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="TX">
<contactref element="NETWORK1" pad="3"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="SERVO_PWM">
<contactref element="SERVO_CONNECTOR1" pad="5"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="NOTICE_LED">
<contactref element="LED3" pad="2"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="SERVO_PWM_2">
<contactref element="SERVO_CONNECTOR1" pad="6"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="HALL_IN">
<contactref element="HALL_CONNECTOR1" pad="2"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R6" pad="2"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="RESETTI">
<contactref element="ISP1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="VSERVO">
<contactref element="SERVO_CONNECTOR1" pad="3"/>
<contactref element="SERVO_CONNECTOR1" pad="4"/>
<contactref element="IC1" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
