<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.1">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="49.53" x2="87.61" y2="49.53" width="0" layer="20"/>
<wire x1="87.61" y1="49.53" x2="87.61" y2="86.03" width="0" layer="20"/>
<wire x1="87.61" y1="86.03" x2="22.86" y2="86.03" width="0" layer="20"/>
<wire x1="22.86" y1="86.03" x2="22.86" y2="49.53" width="0" layer="20"/>
<wire x1="22.86" y1="86.36" x2="22.86" y2="49.53" width="1.27" layer="46"/>
<wire x1="22.86" y1="49.53" x2="87.63" y2="49.53" width="1.27" layer="46"/>
<wire x1="87.63" y1="49.53" x2="87.63" y2="86.36" width="1.27" layer="46"/>
<wire x1="87.63" y1="86.36" x2="22.86" y2="86.36" width="1.27" layer="46"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
<library name="fab2">
<packages>
<package name="2X02SMD">
</package>
</packages>
</library>
<library name="regulators">
<packages>
<package name="SOT-23-3">
<description>SOT-23, 3-pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C_IN" library="fab" package="C1206FAB" value="0.1uF"/>
<element name="LEDPOWER" library="fab" package="LED1206FAB" value="RED"/>
<element name="LEDPOWER_RES" library="fab" package="R1206FAB" value="499"/>
<element name="POWER" library="fab" package="2X02SMD" value=""/>
<element name="PULLUP_3" library="fab" package="R1206FAB" value="10K"/>
<element name="PULLUP_4" library="fab" package="R1206FAB" value="10K"/>
<element name="TWI_IN" library="fab2" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="TWI_OUT1" library="fab2" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="TWI_OUT2" library="fab2" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="TWI_OUT3" library="fab2" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U1" library="regulators" package="SOT-23-3" value="LM3480-5.0"/>
<element name="JUMPER" library="fab" package="R1206FAB" value="0"/>
<element name="JUMPER1" library="fab" package="R1206FAB" value="0"/>
<element name="JUMPER2" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LEDPOWER_RES" pad="2"/>
<contactref element="POWER" pad="4"/>
<contactref element="POWER" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="C_IN" pad="2"/>
<contactref element="TWI_IN" pad="4"/>
<contactref element="TWI_OUT1" pad="4"/>
<contactref element="TWI_OUT2" pad="4"/>
<contactref element="TWI_OUT3" pad="4"/>
<contactref element="JUMPER" pad="2"/>
<contactref element="JUMPER1" pad="2"/>
<contactref element="JUMPER2" pad="2"/>
<contactref element="JUMPER" pad="1"/>
<contactref element="JUMPER1" pad="1"/>
<contactref element="JUMPER2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="LEDPOWER" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="PULLUP_3" pad="2"/>
<contactref element="PULLUP_4" pad="2"/>
<contactref element="TWI_IN" pad="2"/>
<contactref element="TWI_OUT1" pad="2"/>
<contactref element="TWI_OUT2" pad="2"/>
<contactref element="TWI_OUT3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LEDPOWER_RES" pad="1"/>
<contactref element="LEDPOWER" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="TWI_IN" pad="1"/>
<contactref element="PULLUP_3" pad="1"/>
<contactref element="TWI_OUT1" pad="1"/>
<contactref element="TWI_OUT2" pad="1"/>
<contactref element="TWI_OUT3" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="PULLUP_4" pad="1"/>
<contactref element="TWI_IN" pad="3"/>
<contactref element="TWI_OUT1" pad="3"/>
<contactref element="TWI_OUT2" pad="3"/>
<contactref element="TWI_OUT3" pad="3"/>
</signal>
<signal name="V+">
<contactref element="U1" pad="2"/>
<contactref element="C_IN" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="POWER" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
