<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X02SMD">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI"/>
<element name="U$2" library="fab" package="LED1206" value="LED"/>
<element name="10K" library="fab" package="R1206FAB" value=""/>
<element name="1K" library="fab" package="R1206FAB" value=""/>
<element name="1UF" library="fab" package="R1206FAB" value=""/>
<element name="U$4" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
</elements>
<signals>
<signal name="RST">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="10K" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="U$4" pad="1"/>
<contactref element="1UF" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="V">
<contactref element="JP1" pad="5"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$1" pad="8"/>
<contactref element="1UF" pad="1"/>
<contactref element="10K" pad="2"/>
<contactref element="1K" pad="2"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="TXD">
<contactref element="U$4" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="U$4" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="1K">
<contactref element="1K" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="U$3" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="U$3" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
