(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 25)
    (no_connects 1)
    (area 124.61 85.01819 167.215001 116.251809)
    (thickness 1.6)
    (drawings 0)
    (tracks 86)
    (zones 0)
    (modules 11)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 VCC)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(IC1-Pad1)")
  (net 6 "Net-(IC1-Pad2)")
  (net 7 "Net-(IC1-Pad5)")
  (net 8 "Net-(IC1-Pad6)")
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(JP1-Pad2)")
  (net 11 "Net-(JP1-Pad4)")
  (net 12 "Net-(JP1-Pad6)")
  (net 13 "Net-(MIC1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP1-Pad4)")
    (add_net "Net-(JP1-Pad6)")
    (add_net "Net-(MIC1-Pad2)")
    (add_net VCC)
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 153.58 106.17 270)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778 270) (layer F.SilkS))
    (fp_text value CAP-UNPOLARIZEDFAB (at 1.27 1.778 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 131.81 95.1 90)
    (attr smd)
    (fp_text reference C2 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value CAP-UNPOLARIZEDFAB (at 1.27 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 144.07 93.82)
    (attr smd)
    (fp_text reference C3 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value CAP-UNPOLARIZEDFAB (at 1.27 1.778) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 150.37 95.33 90)
    (attr smd)
    (fp_text reference C4 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value CAP-UNPOLARIZEDFAB (at 1.27 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-SOIC8 (layer F.Cu) (tedit 200000)
    (at 144.67 104.66 180)
    (descr "WIDE PLASTIC GULL WING SMALL OUTLINE PACKAGE")
    (tags "WIDE PLASTIC GULL WING SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -3.4925 -1.016 270) (layer F.SilkS))
    (fp_text value ATTINY45SI (at 3.429 -1.651 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.905 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -0.64262 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at 0.62484 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at 1.89484 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 5 smd rect (at 1.905 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 0.635 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -0.635 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -1.905 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 135.51 104.72 180)
    (attr smd)
    (fp_text reference J1 (at -0.635 -4.445 180) (layer F.SilkS))
    (fp_text value AVRISP (at 0 4.445 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 2 smd rect (at 2.91846 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -2.54 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 4 smd rect (at 2.91846 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 5 smd rect (at -2.54 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 6 smd rect (at 2.91846 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 158.76 96.25)
    (attr smd)
    (fp_text reference JP1 (at -0.635 -4.445) (layer F.SilkS))
    (fp_text value PINHD-2X3-SMD (at 0 4.445) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 2.91846 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(JP1-Pad2)"))
    (pad 3 smd rect (at -2.54 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 2.91846 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(JP1-Pad4)"))
    (pad 5 smd rect (at -2.54 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at 2.91846 2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(JP1-Pad6)"))
  )
  (module fab:fab-MIC_MEMS_ANALOG_SPU0414HR5H (layer F.Cu) (tedit 200000)
    (at 137.27 95.23)
    (descr HTTP://WWW.DIGIKEY.COM/PRODUCT-SEARCH/EN?KEYWORDS=423-1134-1-ND%09)
    (tags HTTP://WWW.DIGIKEY.COM/PRODUCT-SEARCH/EN?KEYWORDS=423-1134-1-ND%09)
    (attr smd)
    (fp_text reference MIC1 (at 0.59436 -3.03784) (layer F.SilkS))
    (fp_text value MIC_MEMS_ANALOG (at 1.09474 3.05562) (layer F.SilkS))
    (pad 1 smd circle (at 0.9652 -1.3716) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd circle (at 0.9652 1.3716) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(MIC1-Pad2)"))
    (pad 3 smd circle (at -0.9652 1.3716) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd circle (at -0.9652 -1.3716) (size 1.143 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 150 106.06 270)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778 270) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.778 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 144.12 96.89)
    (attr smd)
    (fp_text reference R2 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.778) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(MIC1-Pad2)"))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 129.42 99.41)
    (attr smd)
    (fp_text reference R4 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value jumper (at 1.27 1.778) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.84 89.63) (xy 165.07 89.74) (xy 164.85 113.66) (xy 124.61 113.16)
      )
    )
  )
)
