(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 32)
    (no_connects 2)
    (area 99 61.4 168.400001 112.200001)
    (thickness 1.6)
    (drawings 1)
    (tracks 123)
    (zones 0)
    (modules 14)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 VCC)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad4)")
  (net 7 "Net-(IC1-Pad5)")
  (net 8 "Net-(IC1-Pad6)")
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(IC1-Pad8)")
  (net 11 "Net-(IC1-Pad9)")
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad12)")
  (net 15 "Net-(IC1-Pad13)")
  (net 16 "Net-(LED1-PadB)")
  (net 17 "Net-(LED1-PadG)")
  (net 18 "Net-(LED1-PadR)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(LED1-PadB)")
    (add_net "Net-(LED1-PadG)")
    (add_net "Net-(LED1-PadR)")
    (add_net VCC)
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 58F270D9)
    (at 109.8 89 90)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value CAP-US1206 (at 2.54 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 90) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.39954 0 90) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 114.4 89 270)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C2 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value CAP-US1206 (at 2.54 1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 270) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.39954 0 270) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 137 83 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143 360) (layer F.SilkS))
    (fp_text value ATTINY44-SSU (at 1.27 0.0635 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-SOT23 (layer F.Cu) (tedit 200000)
    (at 119.81 88.79 180)
    (descr "SOT 23")
    (tags "SOT 23")
    (attr smd)
    (fp_text reference IC2 (at 1.27 -2.54 180) (layer F.SilkS))
    (fp_text value REGULATORSOT23 (at 1.905 2.54 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.94996 1.09982 180) (size 0.99822 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.94996 1.09982 180) (size 0.99822 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 0 -1.09982 180) (size 0.99822 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-P-LCC-4 (layer F.Cu) (tedit 200000)
    (at 157.71 94.77)
    (descr "POWER TOPLED®")
    (tags "POWER TOPLED®")
    (attr smd)
    (fp_text reference LED1 (at -4.445 -0.635 90) (layer F.SilkS))
    (fp_text value LEDRGBNEW (at 4.445 -1.27 90) (layer F.SilkS))
    (fp_text user R (at -1.27 3.175) (layer F.SilkS))
    (fp_text user G (at -1.27 -3.175) (layer F.SilkS))
    (fp_text user B (at 1.905 -3.175) (layer F.SilkS))
    (fp_text user A (at 1.905 3.175) (layer F.SilkS))
    (pad A smd rect (at 1.99898 3.1496) (size 3.29946 4.79806) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad B smd rect (at 1.99898 -3.1496) (size 3.29946 4.79806) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED1-PadB)"))
    (pad G smd rect (at -1.99898 -3.1496) (size 3.29946 4.79806) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED1-PadG)"))
    (pad R smd rect (at -1.99898 3.1496) (size 3.29946 4.79806) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-PadR)"))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 127 80.5 270)
    (attr smd)
    (fp_text reference M1 (at 0 0 270) (layer F.SilkS))
    (fp_text value RESONATOR (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad3)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 111.4 83.2 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value RES-US1206 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 148.6 87.8 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value RES-US1206 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED1-PadB)"))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad12)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 148.6 94.8 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R3 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value RES-US1206 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(LED1-PadR)"))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad10)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 148.6 91.2 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R4 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value RES-US1206 (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(LED1-PadG)"))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 106.8 93.6 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R5 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value jumper (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 133.2 97.4 180)
    (attr smd)
    (fp_text reference ISP1 (at -0.635 -4.445 180) (layer F.SilkS))
    (fp_text value AVRISP (at 0 4.445 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad8)"))
    (pad 2 smd rect (at 2.91846 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -2.54 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 4 smd rect (at 2.91846 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 5 smd rect (at -2.54 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad4)"))
    (pad 6 smd rect (at 2.91846 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 120 95.8)
    (attr smd)
    (fp_text reference JP1 (at -0.635 -3.175) (layer F.SilkS))
    (fp_text value PINHD-2X2-SMD (at 0 3.175) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad5)"))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad6)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 134.4 76.4)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R6 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value jumper (at 2.54 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (gr_text "RGB LED  |  ANA CABRAL  |  2017" (at 132 69) (layer F.Cu))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.2 63) (xy 168.4 61.4) (xy 168.4 112.2) (xy 99 111.4) (xy 100.8 63.4)
      )
    )
  )
)
