<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.42" y2="0" width="0" layer="20"/>
<wire x1="31.42" y1="0" x2="31.42" y2="20.31" width="0" layer="20"/>
<wire x1="31.42" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>iMidoriNY</text>
<text>Smartbeddo</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="USB_MINIB">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="fab" package="USB_MINIB" value="USB_MINIB"/>
<element name="U$2" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="D+"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="D-"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="VBUS"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="GND"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
