PCBNEW-BOARD Version 1 date mié 18 abr 2012 08:09:22 CEST

# Created by Pcbnew(2011-11-15 BZR 3235)-stable

$GENERAL
encoding utf-8
LayerCount 2
Ly 1FFF8001
EnabledLayers 1FFF8001
Links 9
NoConn 0
Di 51599 33099 63401 39901
Ndraw 8
Ntrack 34
Nzone 0
BoardThickness 630
Nmodule 5
Nnets 6
$EndGENERAL

$SHEETDESCR
Sheet A4 11700 8267
Title ""
Date "18 apr 2012"
Rev ""
Comp ""
Comment1 ""
Comment2 ""
Comment3 ""
Comment4 ""
$EndSHEETDESCR

$SETUP
InternalUnit 0.000100 INCH
Layers 2
Layer[0] Back signal
Layer[15] Front signal
TrackWidth 119
TrackClearence 100
ZoneClearence 200
TrackMinWidth 80
DrawSegmWidth 150
EdgeSegmWidth 150
ViaSize 350
ViaDrill 200
ViaMinSize 350
ViaMinDrill 200
MicroViaSize 200
MicroViaDrill 50
MicroViasAllowed 0
MicroViaMinSize 200
MicroViaMinDrill 50
TextPcbWidth 120
TextPcbSize 600 800
EdgeModWidth 150
TextModSize 600 600
TextModWidth 120
PadSize 600 600
PadDrill 320
Pad2MaskClearance 100
AuxiliaryAxisOrg 0 0
PcbPlotParams (pcbplotparams (layerselection 32768) (usegerberextensions true) (excludeedgelayer false) (linewidth 60) (plotframeref false) (viasonmask false) (mode 1) (useauxorigin false) (hpglpennumber 1) (hpglpenspeed 20) (hpglpendiameter 15) (hpglpenoverlay 2) (pscolor true) (psnegative false) (psa4output false) (plotreference true) (plotvalue true) (plotothertext true) (plotinvisibletext false) (padsonsilk false) (subtractmaskfromsilk false) (outputformat 2) (mirror true) (drillshape 1) (scaleselection 1) (outputdirectory ""))
$EndSETUP

$EQUIPOT
Na 0 ""
St ~
$EndEQUIPOT
$EQUIPOT
Na 1 "GND"
St ~
$EndEQUIPOT
$EQUIPOT
Na 2 "LED"
St ~
$EndEQUIPOT
$EQUIPOT
Na 3 "N-000003"
St ~
$EndEQUIPOT
$EQUIPOT
Na 4 "SPK"
St ~
$EndEQUIPOT
$EQUIPOT
Na 5 "VCC"
St ~
$EndEQUIPOT
$NCLASS
Name "Default"
Desc "This is the default net class."
Clearance 100.000000
TrackWidth 119.000000
ViaDia 350.000000
ViaDrill 200.000000
uViaDia 200.000000
uViaDrill 50.000000
AddNet ""
AddNet "GND"
AddNet "LED"
AddNet "N-000003"
AddNet "SPK"
AddNet "VCC"
$EndNCLASS
$MODULE SM0805
Po 59000 34000 1800 15 42806E04 4F8E587C ~~
Li SM0805
Sc 4F8E587C
AR /4F8E5777
Op 0 0 0
At SMD 
T0 0 0 250 250 1800 50 N V 21 N "R1"
T1 0 0 250 250 1800 50 N I 21 N "R"
DC -650 300 -650 250 50 21
DS -200 300 -600 300 50 21
DS -600 300 -600 -300 50 21
DS -600 -300 -200 -300 50 21
DS 200 -300 600 -300 50 21
DS 600 -300 600 300 50 21
DS 600 300 200 300 50 21
$PAD
Sh "1" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 5 "VCC"
Po -375 0
$EndPAD
$PAD
Sh "2" R 350 550 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po 375 0
$EndPAD
$SHAPE3D
Na "smd/chip_cms.wrl"
Sc 0.100000 0.100000 0.100000
Of 0.000000 0.000000 0.000000
Ro 0.000000 0.000000 0.000000
$EndSHAPE3D
$EndMODULE  SM0805
$MODULE LED-1206
Po 57500 34750 2700 15 49BFA1FF 4F8E587D ~~
Li LED-1206
Cd LED 1206 smd package
Kw LED1206 SMD
Sc 4F8E587D
AR /4F8E577E
Op 0 0 0
At SMD 
T0 100 -600 300 300 2700 35 N V 21 N "D1"
T1 0 600 300 300 2700 35 N V 21 N "LED"
DS -39 39 39 39 26 21
DS 39 39 39 -39 26 21
DS -39 -39 39 -39 26 21
DS -39 39 -39 -39 26 21
DS 177 275 314 275 26 21
DS 314 275 314 177 26 21
DS 177 177 314 177 26 21
DS 177 275 177 177 26 21
DS 314 275 354 275 26 21
DS 354 275 354 -196 26 21
DS 314 -196 354 -196 26 21
DS 314 275 314 -196 26 21
DS 314 -216 354 -216 26 21
DS 354 -216 354 -275 26 21
DS 314 -275 354 -275 26 21
DS 314 -216 314 -275 26 21
DS -354 275 -314 275 26 21
DS -314 275 -314 -196 26 21
DS -354 -196 -314 -196 26 21
DS -354 275 -354 -196 26 21
DS -354 -216 -314 -216 26 21
DS -314 -216 -314 -275 26 21
DS -354 -275 -314 -275 26 21
DS -354 -216 -354 -275 26 21
DS 177 275 236 275 26 21
DS 236 275 236 177 26 21
DS 177 177 236 177 26 21
DS 177 275 177 177 26 21
DS 610 295 -610 295 40 21
DS -610 295 -610 -295 40 21
DS -610 -295 610 -295 40 21
DS 610 -295 610 295 40 21
DA 0 0 216 196 954 40 21
DA 0 0 -216 196 845 40 21
DA 0 0 -216 -196 954 40 21
DA 0 0 216 -196 845 40 21
$PAD
Sh "1" R 629 709 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 3 "N-000003"
Po -559 0
$EndPAD
$PAD
Sh "2" R 629 709 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 2 "LED"
Po 559 0
$EndPAD
$EndMODULE  LED-1206
$MODULE CONN-4-SMD
Po 54500 35500 900 15 4F82EAB7 4F8E587E ~~
Li CONN-4-SMD
Sc 4F8E587E
AR /4F8E56D8
Op 0 0 0
T0 0 -2000 354 354 900 79 N V 21 N "P1"
T1 0 -1000 472 551 900 79 N V 21 N "IN"
DS 2000 -1500 -2000 -1500 150 21
DS -2000 -2500 2000 -2500 150 21
DS -2000 -2500 -2000 -1500 150 21
DS 2000 -1500 2000 -2500 150 21
$PAD
Sh "1" R 394 1181 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 5 "VCC"
Po -1500 0
$EndPAD
$PAD
Sh "2" R 394 1181 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 2 "LED"
Po -500 0
$EndPAD
$PAD
Sh "3" R 394 1181 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 4 "SPK"
Po 500 0
$EndPAD
$PAD
Sh "4" R 394 1181 0 0 900
Dr 0 0 0
At SMD N 00888000
Ne 1 "GND"
Po 1500 0
$EndPAD
$EndMODULE  CONN-4-SMD
$MODULE CONN-4-SMD
Po 60500 35500 2700 15 4F82EAB7 4F8E5880 ~~
Li CONN-4-SMD
Sc 4F8E5880
AR /4F8E56D3
Op 0 0 0
T0 0 -2000 354 354 2700 79 N V 21 N "P2"
T1 0 -1000 472 551 2700 79 N V 21 N "OUT"
DS 2000 -1500 -2000 -1500 150 21
DS -2000 -2500 2000 -2500 150 21
DS -2000 -2500 -2000 -1500 150 21
DS 2000 -1500 2000 -2500 150 21
$PAD
Sh "1" R 394 1181 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 5 "VCC"
Po -1500 0
$EndPAD
$PAD
Sh "2" R 394 1181 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 2 "LED"
Po -500 0
$EndPAD
$PAD
Sh "3" R 394 1181 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 4 "SPK"
Po 500 0
$EndPAD
$PAD
Sh "4" R 394 1181 0 0 2700
Dr 0 0 0
At SMD N 00888000
Ne 1 "GND"
Po 1500 0
$EndPAD
$EndMODULE  CONN-4-SMD
$MODULE CONN-2-SMD
Po 57500 37000 1800 15 4F8E589D 4F8E5881 ~~
Li CONN-2-SMD
Sc 4F8E5881
AR /4F8E578D
Op 0 0 0
T0 0 -2000 354 354 1800 79 N V 21 N "P3"
T1 0 -1000 472 551 1800 79 N V 21 N "CONN_2"
DS -900 -1500 900 -1500 150 21
DS -900 -2500 900 -2500 150 21
DS -900 -2500 -900 -1500 150 21
DS 900 -1500 900 -2500 150 21
$PAD
Sh "1" R 394 1181 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 5 "VCC"
Po -500 0
$EndPAD
$PAD
Sh "2" R 394 1181 0 0 1800
Dr 0 0 0
At SMD N 00888000
Ne 4 "SPK"
Po 500 0
$EndPAD
$EndMODULE  CONN-2-SMD
$TEXTPCB
Te "David Pello 2012"
Po 61000 38750 236 236 39 0
De 15 1 0 Normal C
$EndTEXTPCB
$TEXTPCB
Te "Beacon"
Po 60500 38250 394 394 79 0
De 15 1 0 Normal C
$EndTEXTPCB
$TEXTPCB
Te "OpenHAB"
Po 53750 38750 394 394 79 0
De 15 1 0 Normal C
$EndTEXTPCB
$DRAWSEGMENT
Po 0 63250 33250 51750 33250 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 63250 39750 63250 33250 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 51750 39750 63250 39750 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 51750 39500 51750 39750 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$DRAWSEGMENT
Po 0 51750 33250 51750 39500 150
De 28 0 900 0 0
$EndDRAWSEGMENT
$TRACK
Po 0 57500 35309 56191 35309 119 -1
De 15 0 2 0 400000
Po 0 56191 35309 55500 36000 119 -1
De 15 0 2 0 0
Po 0 55500 36000 54500 36000 119 -1
De 15 0 2 0 800000
Po 0 54500 36000 55500 36000 119 -1
De 15 0 2 0 400000
Po 0 59250 35000 60500 35000 119 -1
De 15 0 2 0 800000
Po 0 58941 35309 59250 35000 119 -1
De 15 0 2 0 0
Po 0 56191 35309 58941 35309 119 -1
De 15 0 2 0 0
Po 0 55500 36000 56191 35309 119 -1
De 15 0 2 0 0
Po 0 58625 34000 57941 34000 119 -1
De 15 0 3 0 400000
Po 0 57941 34000 57750 34191 119 -1
De 15 0 3 0 800000
Po 0 57750 34191 57500 34191 119 -1
De 15 0 3 0 C00000
Po 0 57941 34000 57500 34441 119 -1
De 15 0 3 0 0
Po 0 57000 37000 57000 36500 119 -1
De 15 0 4 0 C00000
Po 0 57500 36000 60500 36000 119 -1
De 15 0 4 0 800000
Po 0 57000 36500 57500 36000 119 -1
De 15 0 4 0 400000
Po 0 56000 36500 56500 37000 119 -1
De 15 0 4 0 0
Po 0 53750 35000 53500 35250 119 -1
De 15 0 4 0 0
Po 0 53500 35250 53500 36250 119 -1
De 15 0 4 0 0
Po 0 53500 36250 53750 36500 119 -1
De 15 0 4 0 0
Po 0 53750 36500 56000 36500 119 -1
De 15 0 4 0 0
Po 0 56500 37000 57000 37000 119 -1
De 15 0 4 0 800000
Po 0 54500 35000 53750 35000 119 -1
De 15 0 4 0 400000
Po 0 58000 37000 58250 37000 119 -1
De 15 0 5 0 400000
Po 0 61000 34000 60500 34000 119 -1
De 15 0 5 0 C00000
Po 0 61500 34500 61000 34000 119 -1
De 15 0 5 0 800000
Po 0 61500 36250 61500 34500 119 -1
De 15 0 5 0 0
Po 0 61250 36500 61500 36250 119 -1
De 15 0 5 0 0
Po 0 58750 36500 61250 36500 119 -1
De 15 0 5 0 0
Po 0 58250 37000 58750 36500 119 -1
De 15 0 5 0 0
Po 0 59375 34000 60500 34000 119 -1
De 15 0 5 0 C00000
Po 0 54500 37000 56000 38500 119 -1
De 15 0 5 0 400000
Po 0 58000 38000 58000 37000 119 -1
De 15 0 5 0 800000
Po 0 57500 38500 58000 38000 119 -1
De 15 0 5 0 0
Po 0 56000 38500 57500 38500 119 -1
De 15 0 5 0 0
$EndTRACK
$ZONE
$EndZONE
$CZONE_OUTLINE
ZInfo 4F8E599C 1 "GND"
ZLayer 15
ZAux 4 E
ZClearance 200 T
ZMinThickness 100
ZOptions 0 16 F 200 200
ZSmoothing 0 0
ZCorner 63250 39750 0
ZCorner 63250 33250 0
ZCorner 51750 33250 0
ZCorner 51750 39750 1
$POLYSCORNERS
62925 39425 0 0
62827 39425 0 0
62827 39185 0 0
62827 38278 0 0
61858 38278 0 0
61858 37607 0 0
61340 37607 0 0
61340 37112 0 0
61278 37050 0 0
60550 37050 0 0
60550 37385 0 0
60612 37447 0 0
61041 37446 0 0
61140 37446 0 0
61231 37408 0 0
61301 37338 0 0
61339 37246 0 0
61340 37112 0 0
61340 37607 0 0
60450 37607 0 0
60450 37385 0 0
60450 37050 0 0
59722 37050 0 0
59660 37112 0 0
59661 37246 0 0
59699 37338 0 0
59769 37408 0 0
59860 37446 0 0
59959 37446 0 0
60388 37447 0 0
60450 37385 0 0
60450 37607 0 0
59142 37607 0 0
59142 38815 0 0
59173 38815 0 0
59173 39185 0 0
62827 39185 0 0
62827 39425 0 0
52075 39425 0 0
52075 33575 0 0
53809 33575 0 0
53769 33592 0 0
53699 33662 0 0
53661 33754 0 0
53660 33888 0 0
53722 33950 0 0
54400 33950 0 0
54450 33950 0 0
54550 33950 0 0
54600 33950 0 0
55278 33950 0 0
55340 33888 0 0
55339 33754 0 0
55301 33662 0 0
55231 33592 0 0
55190 33575 0 0
58248 33575 0 0
58239 33584 0 0
58201 33675 0 0
58201 33691 0 0
58020 33691 0 0
57995 33666 0 0
57904 33628 0 0
57805 33628 0 0
57097 33628 0 0
57005 33666 0 0
56935 33736 0 0
56897 33827 0 0
56897 33926 0 0
56897 34554 0 0
56935 34646 0 0
57005 34716 0 0
57086 34750 0 0
57005 34784 0 0
56935 34854 0 0
56897 34945 0 0
56897 35000 0 0
56191 35000 0 0
56073 35024 0 0
55972 35091 0 0
55372 35691 0 0
55340 35691 0 0
55340 34112 0 0
55278 34050 0 0
54550 34050 0 0
54550 34385 0 0
54612 34447 0 0
55041 34446 0 0
55140 34446 0 0
55231 34408 0 0
55301 34338 0 0
55339 34246 0 0
55340 34112 0 0
55340 35691 0 0
55312 35691 0 0
55301 35662 0 0
55231 35592 0 0
55140 35554 0 0
55041 35554 0 0
53861 35554 0 0
53809 35575 0 0
53809 35424 0 0
53860 35446 0 0
53959 35446 0 0
55139 35446 0 0
55231 35408 0 0
55301 35338 0 0
55339 35247 0 0
55339 35148 0 0
55339 34754 0 0
55301 34662 0 0
55231 34592 0 0
55140 34554 0 0
55041 34554 0 0
54450 34554 0 0
54450 34385 0 0
54450 34050 0 0
53722 34050 0 0
53660 34112 0 0
53661 34246 0 0
53699 34338 0 0
53769 34408 0 0
53860 34446 0 0
53959 34446 0 0
54388 34447 0 0
54450 34385 0 0
54450 34554 0 0
53861 34554 0 0
53769 34592 0 0
53699 34662 0 0
53681 34705 0 0
53680 34705 0 0
53632 34715 0 0
53531 34782 0 0
53282 35032 0 0
53215 35132 0 0
53191 35250 0 0
53191 36250 0 0
53215 36368 0 0
53282 36468 0 0
53531 36718 0 0
53532 36718 0 0
53632 36785 0 0
53661 36790 0 0
53661 36852 0 0
53661 37246 0 0
53699 37338 0 0
53769 37408 0 0
53860 37446 0 0
53959 37446 0 0
54509 37446 0 0
55170 38107 0 0
52157 38107 0 0
52157 39315 0 0
55343 39315 0 0
55343 38279 0 0
55781 38718 0 0
55782 38718 0 0
55882 38785 0 0
56000 38809 0 0
57500 38809 0 0
57500 38808 0 0
57618 38785 0 0
57718 38718 0 0
58218 38219 0 0
58218 38218 0 0
58285 38118 0 0
58308 38000 0 0
58309 38000 0 0
58309 37812 0 0
58338 37801 0 0
58408 37731 0 0
58446 37640 0 0
58446 37541 0 0
58446 37232 0 0
58468 37218 0 0
58877 36809 0 0
59660 36809 0 0
59660 36888 0 0
59722 36950 0 0
60400 36950 0 0
60450 36950 0 0
60550 36950 0 0
60600 36950 0 0
61278 36950 0 0
61340 36888 0 0
61339 36790 0 0
61368 36785 0 0
61468 36718 0 0
61718 36469 0 0
61718 36468 0 0
61785 36368 0 0
61808 36250 0 0
61809 36250 0 0
61809 34500 0 0
61785 34382 0 0
61718 34282 0 0
61718 34281 0 0
61339 33902 0 0
61339 33754 0 0
61301 33662 0 0
61231 33592 0 0
61190 33575 0 0
62925 33575 0 0
62925 39425 1 0
$endPOLYSCORNERS
$endCZONE_OUTLINE
$EndBOARD
