<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="21.59" y1="1.27" x2="51.74" y2="1.27" width="0" layer="20"/>
<wire x1="51.74" y1="1.27" x2="51.74" y2="31.74" width="0" layer="20"/>
<wire x1="51.74" y1="31.74" x2="21.59" y2="31.74" width="0" layer="20"/>
<wire x1="21.59" y1="31.74" x2="21.59" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_LONGPADS">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GND" library="01_SparkFun" package="1X05_LONGPADS" value=""/>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="POWER" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="VCC_5V" library="01_SparkFun" package="1X05_LONGPADS" value=""/>
<element name="VCC_3.3V" library="01_SparkFun" package="1X05_LONGPADS" value=""/>
<element name="UA78M33C" library="linear" package="TO220V" value="7805TV"/>
<element name="C3" library="01_SparkFun" package="1206" value="10uF"/>
<element name="C1" library="01_SparkFun" package="1206" value="10uF"/>
<element name="C2" library="01_SparkFun" package="1206" value="10uF"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="VCC_5V" pad="1"/>
<contactref element="VCC_5V" pad="2"/>
<contactref element="VCC_5V" pad="3"/>
<contactref element="VCC_5V" pad="4"/>
<contactref element="VCC_5V" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="1"/>
<contactref element="POWER" pad="2"/>
<contactref element="UA78M33C" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="UA78M33C" pad="3"/>
<contactref element="VCC_3.3V" pad="5"/>
<contactref element="VCC_3.3V" pad="4"/>
<contactref element="VCC_3.3V" pad="3"/>
<contactref element="VCC_3.3V" pad="2"/>
<contactref element="VCC_3.3V" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="2"/>
<contactref element="GND" pad="4"/>
<contactref element="GND" pad="3"/>
<contactref element="GND" pad="5"/>
<contactref element="GND" pad="1"/>
<contactref element="GND" pad="2"/>
<contactref element="UA78M33C" pad="2"/>
<contactref element="POWER" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
