<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="63.5" x2="33.325" y2="63.5" width="0" layer="20"/>
<wire x1="33.325" y1="63.5" x2="33.325" y2="78.73" width="0" layer="20"/>
<wire x1="33.325" y1="78.73" x2="0" y2="78.73" width="0" layer="20"/>
<wire x1="0" y1="78.73" x2="0" y2="63.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="1X01">
</package>
<package name="SWITCH-SPDT">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Zaerc">
<packages>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_SparkFun" package="1206" value="1uF"/>
<element name="C2" library="01_SparkFun" package="1206" value="10uF"/>
<element name="C3" library="01_SparkFun" package="1206" value="10uF"/>
<element name="D1" library="Zaerc" package="MINI-SMA" value="CDBM1100-G"/>
<element name="JP1/GNDFTDI" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="JP2/VCCBAT" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="JP2/VCCFTDI" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="S1" library="01_SparkFun" package="SWITCH-SPDT" value=""/>
<element name="U$1" library="01_SparkFun" package="SOT223" value="V_REG_MIC2920"/>
<element name="JP2/GNDBAT1" library="01_SparkFun" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP2/VCCBAT" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D1" pad="ANODE"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="JP1/GNDFTDI" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP2/GNDBAT1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="KATHODE"/>
<contactref element="JP2/VCCFTDI" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
