<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="47.625" y1="26.67" x2="47.625" y2="34.595" width="0" layer="20"/>
<wire x1="47.625" y1="34.595" x2="29.855" y2="34.595" width="0" layer="20"/>
<wire x1="29.855" y1="34.595" x2="29.855" y2="26.67" width="0" layer="20"/>
<wire x1="29.855" y1="26.67" x2="47.625" y2="26.67" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-SMD">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="01_FAB_Hello" package="1206" value="100"/>
<element name="R3" library="01_FAB_Hello" package="1206" value="100"/>
<element name="R5" library="01_FAB_Hello" package="1206" value="100"/>
<element name="U$1" library="01_SparkFun" package="LED-TRICOLOR-SMD" value="LED-TRICOLOR"/>
<element name="JP1" library="01_SparkFun" package="1X02" value=""/>
<element name="JP2" library="01_SparkFun" package="1X02" value=""/>
</elements>
<signals>
<signal name="LEDB">
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="LEDG">
<contactref element="R5" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="R"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="B"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="G"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="A"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
