<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="26.035" y1="28.067" x2="26.035" y2="0" width="0.2032" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="28.067" width="0.2032" layer="20"/>
<wire x1="0" y1="28.067" x2="26.035" y2="28.067" width="0.2032" layer="20"/>
<wire x1="26.035" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>3V3</text>
<text>TXO</text>
<text>RXI</text>
<text>GND</text>
<text>FTDI Basic</text>
<text>DTR</text>
<text>RX</text>
<text>TX</text>
<text>CTS</text>
<text>Close</text>
<text>5V</text>
<text>BLK</text>
<text>5V</text>
<text>3.3V</text>
<text>GRN</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="EIA3216">
</package>
<package name="SFE-NEW-WEB">
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="USB_MINIB">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="SPDTSWITCH">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun" package="SFE-NEW-WEB" value="LOGO-SFENW2"/>
<element name="U1" library="SparkFun" package="SSOP28DB" value="FT232RLSSOP"/>
<element name="R1" library="fab" package="R1206FAB" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="1206" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="1206" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="SFE-LOGO-FLAME" value="LOGO-SFESK"/>
<element name="JP3" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="U$5" library="01_fab" package="USB_MINIB" value="USB_MINIB"/>
<element name="U$6" library="fab" package="SPDTSWITCH" value="SPDTSWITCH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="21"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$5" pad="GND"/>
</signal>
<signal name="USB_D-">
<contactref element="U1" pad="16"/>
<contactref element="U$5" pad="D-"/>
</signal>
<signal name="USB_D+">
<contactref element="U1" pad="15"/>
<contactref element="U$5" pad="D+"/>
</signal>
<signal name="CTS">
<contactref element="U1" pad="11"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="DTR">
<contactref element="U1" pad="2"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="23"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="22"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="RXI">
<contactref element="U1" pad="5"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="POWER">
<contactref element="U1" pad="4"/>
<contactref element="JP3" pad="3"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="20"/>
<contactref element="C5" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$5" pad="VBUS"/>
<contactref element="U$6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
