<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="25.1" x2="8.1" y2="34.9" width="0.001" layer="20" curve="-90"/>
<wire x1="8.1" y1="34.9" x2="25.9" y2="34.9" width="0.001" layer="20"/>
<wire x1="25.9" y1="34.9" x2="27.2" y2="34.9" width="0.001" layer="20"/>
<wire x1="0" y1="25.1" x2="0" y2="7" width="0.001" layer="20"/>
<wire x1="7" y1="0" x2="31.3" y2="0" width="0.001" layer="20"/>
<wire x1="31.3" y1="0" x2="33.8" y2="2.5" width="0.001" layer="20" curve="90"/>
<wire x1="33.8" y1="2.5" x2="33.8" y2="10.7" width="0.001" layer="20"/>
<wire x1="7" y1="0" x2="0" y2="7" width="0.001" layer="20" curve="-90"/>
<text>Snader</text>
<wire x1="32.6" y1="28.3" x2="30.4" y2="28.3" width="0.001" layer="20"/>
<wire x1="30.4" y1="28.3" x2="30.4" y2="11.9" width="0.001" layer="20"/>
<wire x1="32.6" y1="11.9" x2="30.4" y2="11.9" width="0.001" layer="20"/>
<wire x1="32.6" y1="11.9" x2="33.8" y2="10.7" width="0.001" layer="20" curve="-90"/>
<wire x1="32.6" y1="28.3" x2="33.8" y2="29.5" width="0.001" layer="20" curve="90"/>
<wire x1="33.8" y1="29.5" x2="28.4" y2="34.9" width="0.001" layer="20" curve="90"/>
<wire x1="28.4" y1="34.9" x2="27.2" y2="34.9" width="0.001" layer="20"/>
</plain>
<libraries>
<library name="00fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="EFOBM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="00fab" package="SOIC14" value="ATTINY44-SSU">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U$1" library="00fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="FTDIHEADER" library="00fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="C1" library="00fab" package="C1206FAB" value="1uF">
<attribute name="OC_FARNELL" value="1301811"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="12065C105KAT2A"/>
</element>
<element name="R1" library="00fab" package="R1206FAB" value="10k">
<attribute name="OC_FARNELL" value="2073878"/>
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCMR12X1002FTL"/>
</element>
<element name="U$2" library="00fab" package="EFOBM" value="RESONATOR">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U$3" library="00fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R2" library="00fab" package="R1206FAB" value="100">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="BUTTON" library="00fab" package="6MM_SWITCH" value="1">
<attribute name="OC_FARNELL" value="2076274"/>
<attribute name="MF" value="OMRON ELECTRONIC COMPONENTS"/>
<attribute name="MPN" value="B3SN-3112P"/>
</element>
<element name="R3" library="00fab" package="R1206FAB" value="10k">
<attribute name="OC_FARNELL" value="2073878"/>
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCMR12X1002FTL"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="FTDIHEADER" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="BUTTON" pad="3"/>
<contactref element="BUTTON" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="FTDIHEADER" pad="3"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RX">
<contactref element="FTDIHEADER" pad="5"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
<contactref element="FTDIHEADER" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="IC1" pad="10"/>
<contactref element="BUTTON" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="BUTTON" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="LEDPIN">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
