<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="16.2052" y1="-8.4074" x2="68.123" y2="-8.3439" width="0" layer="20"/>
<wire x1="68.123" y1="-8.3439" x2="68.123" y2="39.868" width="0" layer="20"/>
<wire x1="68.123" y1="39.868" x2="16.2052" y2="39.8045" width="0" layer="20"/>
<wire x1="16.2052" y1="39.8045" x2="16.2052" y2="-8.4074" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X09_LONGPADS">
</package>
<package name="1X14-LONGPADS">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_adafruit">
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PADS_1" library="01_SparkFun" package="1X09_LONGPADS" value="M09LONGPADS"/>
<element name="PADS_2" library="01_SparkFun" package="1X14-LONGPADS" value="M14LONGPADS"/>
<element name="JP2" library="fab" package="2X03SMD" value=""/>
<element name="PADS_3" library="01_SparkFun" package="1X09_LONGPADS" value="M09LONGPADS"/>
<element name="PADS_4" library="01_SparkFun" package="1X14-LONGPADS" value="M14LONGPADS"/>
<element name="GND" library="01_adafruit" package="1X01" value=""/>
<element name="VCC" library="01_adafruit" package="1X01" value=""/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="C1" library="fab" package="C1206" value="CAP-US1206"/>
<element name="LM2940" library="linear" package="SOT223" value="LM340MP-05"/>
<element name="C2" library="fab" package="C1206" value="0.47 uf"/>
<element name="C3" library="fab" package="C1206" value="0.47uf"/>
<element name="GND1" library="01_adafruit" package="1X01" value=""/>
<element name="VCC1" library="01_adafruit" package="1X01" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="3"/>
<contactref element="VCC" pad="1"/>
<contactref element="LM2940" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="LM2940" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="GND1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="JP2" pad="2"/>
<contactref element="PADS_2" pad="9"/>
<contactref element="PADS_4" pad="9"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="4"/>
<contactref element="PADS_1" pad="9"/>
<contactref element="PADS_3" pad="9"/>
</signal>
<signal name="12">
<contactref element="JP2" pad="6"/>
<contactref element="PADS_1" pad="8"/>
<contactref element="PADS_3" pad="8"/>
</signal>
<signal name="11">
<contactref element="PADS_1" pad="7"/>
<contactref element="JP2" pad="3"/>
<contactref element="PADS_3" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="PADS_3" pad="1"/>
<contactref element="PADS_1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="PADS_2" pad="1"/>
<contactref element="PADS_4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="PADS_2" pad="2"/>
<contactref element="PADS_4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="PADS_2" pad="3"/>
<contactref element="PADS_4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="PADS_2" pad="4"/>
<contactref element="PADS_4" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="PADS_2" pad="5"/>
<contactref element="PADS_4" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="PADS_2" pad="6"/>
<contactref element="PADS_4" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="PADS_2" pad="7"/>
<contactref element="PADS_4" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="PADS_2" pad="8"/>
<contactref element="PADS_4" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="PADS_2" pad="10"/>
<contactref element="PADS_4" pad="10"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="PADS_2" pad="11"/>
<contactref element="PADS_4" pad="11"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="PADS_2" pad="12"/>
<contactref element="PADS_4" pad="12"/>
</signal>
<signal name="N$14">
<contactref element="PADS_2" pad="13"/>
<contactref element="PADS_4" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="PADS_2" pad="14"/>
<contactref element="PADS_4" pad="14"/>
</signal>
<signal name="N$16">
<contactref element="PADS_1" pad="2"/>
<contactref element="PADS_3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="PADS_1" pad="3"/>
<contactref element="PADS_3" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="PADS_1" pad="4"/>
<contactref element="PADS_3" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="PADS_1" pad="5"/>
<contactref element="PADS_3" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="PADS_1" pad="6"/>
<contactref element="PADS_3" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="6"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCCIN">
<contactref element="LM2940" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="VCC1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
