<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="8.2804" y1="-19.3802" x2="77.5464" y2="-19.4056" width="0" layer="20"/>
<wire x1="77.5464" y1="-19.4056" x2="77.5972" y2="52.0092" width="0" layer="20"/>
<wire x1="77.5972" y1="52.0092" x2="8.3312" y2="52.06" width="0" layer="20"/>
<wire x1="8.3312" y1="52.06" x2="8.2804" y2="-19.3802" width="0" layer="20"/>
</plain>
<libraries>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC3216X178N">
</package>
</packages>
</library>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="CSM-7X-DU">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;&lt;p&gt;
Source: www.ecsxtal.com .. Crystal 3.6864MHz CSM_7X_DU.PDF</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2X03SMD">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="sot23">
<packages>
<package name="SOT95P237X112-3N">
</package>
</packages>
</library>
<library name="WEIDMULLER-PM5.08_2_90BLK">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="WEIDMULLER_PM5.08_2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="AVX_By_element14_Batch_1" package="CAPC3216X178N" value="22pF">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="10V"/>
</element>
<element name="C2" library="AVX_By_element14_Batch_1" package="CAPC3216X178N" value="22pF">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="10V"/>
</element>
<element name="MICRO" library="atmega8" package="TQFP32-08" value="ATMEGA328P-AU"/>
<element name="CRYSTAL" library="01_FAB_Hello" package="CSM-7X-DU" value="16Mhz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="01_SparkFun" package="1206" value="10k"/>
<element name="SWITCH" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="POWER" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="LED_13" library="01_FAB_Hello" package="1206" value="YELLOW"/>
<element name="LED_GREEN" library="01_FAB_Hello" package="1206" value=""/>
<element name="R2" library="01_SparkFun" package="1206" value="499"/>
<element name="R3" library="01_SparkFun" package="1206" value="499"/>
<element name="C3" library="01_SparkFun" package="1206" value="10uF"/>
<element name="C4" library="01_SparkFun" package="1206" value="1uF"/>
<element name="C5" library="01_SparkFun" package="1206" value="100nF"/>
<element name="C6" library="01_SparkFun" package="1206" value="100nF"/>
<element name="FTDI" library="pinhead" package="1X06/90" value=""/>
<element name="ISP" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="R4" library="01_SparkFun" package="1206" value="4.7k"/>
<element name="DHT22" library="pinhead" package="1X03" value=""/>
<element name="DS18B20" library="pinhead" package="1X03" value="Temp"/>
<element name="LDR" library="con-amp-quick" package="02P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="M1" library="sot23" package="SOT95P237X112-3N" value="IRLML6244TRPBF">
<attribute name="MPN" value="IRLML6244TRPBF"/>
<attribute name="OC_FARNELL" value="1864517"/>
<attribute name="OC_NEWARK" value="84R9705"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</element>
<element name="M2" library="sot23" package="SOT95P237X112-3N" value="IRLML6244TRPBF">
<attribute name="MPN" value="IRLML6244TRPBF"/>
<attribute name="OC_FARNELL" value="1864517"/>
<attribute name="OC_NEWARK" value="84R9705"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</element>
<element name="M3" library="sot23" package="SOT95P237X112-3N" value="IRLML6244TRPBF">
<attribute name="MPN" value="IRLML6244TRPBF"/>
<attribute name="OC_FARNELL" value="1864517"/>
<attribute name="OC_NEWARK" value="84R9705"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</element>
<element name="D_M3" library="fab" package="SOD123" value=""/>
<element name="D_M9" library="fab" package="SOD123" value=""/>
<element name="D_M10" library="fab" package="SOD123" value=""/>
<element name="R6" library="01_SparkFun" package="1206" value="10k"/>
<element name="R7" library="01_SparkFun" package="1206" value="10k"/>
<element name="R8" library="01_SparkFun" package="1206" value="10k"/>
<element name="C7" library="01_SparkFun" package="1206" value="100nF"/>
<element name="C8" library="01_SparkFun" package="1206" value="100nF"/>
<element name="C9" library="01_SparkFun" package="1206" value="100nF"/>
<element name="STEPPER_CONN_1" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="STEPPER_CONN_2" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="STEPPER_CONN_3" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="STEPPER_CONN_4" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="MICRO" pad="4"/>
<contactref element="MICRO" pad="6"/>
<contactref element="MICRO" pad="18"/>
<contactref element="MICRO" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="LED_GREEN" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="FTDI" pad="3"/>
<contactref element="ISP" pad="2"/>
<contactref element="DHT22" pad="3"/>
<contactref element="DS18B20" pad="3"/>
<contactref element="LDR" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="MICRO" pad="7"/>
<contactref element="CRYSTAL" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="MICRO" pad="8"/>
<contactref element="CRYSTAL" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="MICRO" pad="3"/>
<contactref element="MICRO" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="SWITCH" pad="3"/>
<contactref element="SWITCH" pad="4"/>
<contactref element="MICRO" pad="21"/>
<contactref element="POWER" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="FTDI" pad="1"/>
<contactref element="ISP" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="DHT22" pad="1"/>
<contactref element="DS18B20" pad="1"/>
<contactref element="M1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="M2" pad="2"/>
<contactref element="M3" pad="2"/>
<contactref element="STEPPER_CONN_4" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="LED_GREEN" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="LED_13" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="2"/>
<contactref element="SWITCH" pad="1"/>
<contactref element="SWITCH" pad="2"/>
<contactref element="MICRO" pad="29"/>
<contactref element="C6" pad="1"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="N$29">
</signal>
<signal name="CTS">
<contactref element="FTDI" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="FTDI" pad="4"/>
<contactref element="MICRO" pad="31"/>
</signal>
<signal name="RXD">
<contactref element="FTDI" pad="5"/>
<contactref element="MICRO" pad="30"/>
</signal>
<signal name="N$3">
<contactref element="FTDI" pad="6"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="MICRO" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="LED_13" pad="1"/>
<contactref element="MICRO" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="MICRO" pad="15"/>
<contactref element="M3" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="A0">
<contactref element="R4" pad="1"/>
<contactref element="MICRO" pad="23"/>
<contactref element="LDR" pad="2"/>
</signal>
<signal name="D1">
<contactref element="DHT22" pad="2"/>
<contactref element="MICRO" pad="32"/>
</signal>
<signal name="D2">
<contactref element="DS18B20" pad="2"/>
<contactref element="MICRO" pad="1"/>
</signal>
<signal name="M1">
<contactref element="M1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="MICRO" pad="13"/>
</signal>
<signal name="M2">
<contactref element="M2" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="MICRO" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="M1" pad="3"/>
<contactref element="D_M3" pad="ANODE"/>
<contactref element="C7" pad="1"/>
<contactref element="STEPPER_CONN_1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="M2" pad="3"/>
<contactref element="D_M9" pad="ANODE"/>
<contactref element="C8" pad="1"/>
<contactref element="STEPPER_CONN_2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="M3" pad="3"/>
<contactref element="D_M10" pad="ANODE"/>
<contactref element="C9" pad="1"/>
<contactref element="STEPPER_CONN_3" pad="2"/>
</signal>
<signal name="VCC_POWER">
<contactref element="D_M3" pad="CATHODE"/>
<contactref element="C7" pad="2"/>
<contactref element="D_M9" pad="CATHODE"/>
<contactref element="C8" pad="2"/>
<contactref element="D_M10" pad="CATHODE"/>
<contactref element="C9" pad="2"/>
<contactref element="STEPPER_CONN_1" pad="1"/>
<contactref element="STEPPER_CONN_2" pad="1"/>
<contactref element="STEPPER_CONN_3" pad="1"/>
<contactref element="STEPPER_CONN_4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="MICRO" pad="9"/>
</signal>
<signal name="N$8">
<contactref element="MICRO" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
