<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="28.448" y1="4.318" x2="60.63" y2="4.318" width="0.4064" layer="20"/>
<wire x1="60.63" y1="4.318" x2="60.63" y2="39.36" width="0.4064" layer="20"/>
<wire x1="60.63" y1="39.36" x2="28.448" y2="39.36" width="0.4064" layer="20"/>
<wire x1="28.448" y1="39.36" x2="28.448" y2="4.318" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="FabLab">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="ModernDevice">
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="FabLab" package="SOIC8" value="ATTINY45SI"/>
<element name="BUS" library="pinhead" package="1X04" value=""/>
<element name="ISP" library="pinhead" package="1X06" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="PROD_ID" value="CAP-10009"/>
</element>
<element name="LED1" library="ModernDevice" package="LED-1206" value=""/>
<element name="R1" library="SparkFun" package="1206" value="1K"/>
<element name="R2" library="SparkFun" package="1206" value="10K"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="BUS" pad="1"/>
<contactref element="ISP" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="LED1" pad="C"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="2"/>
<contactref element="BUS" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="3"/>
<contactref element="BUS" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="BUS" pad="2"/>
<contactref element="ISP" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
