<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="NRF24L01">
</package>
<package name="SOT230P696X180-4N">
</package>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
<symbols>
<symbol name="NRF24L01">
<pin name="GND"/>
<pin name="CE"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="IRQ"/>
<pin name="MOSI"/>
<pin name="CSN"/>
<pin name="VCC"/>
</symbol>
<symbol name="LM1117MP-3.3">
<pin name="IN" direction="in"/>
<pin name="ADJ/GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ATMEGA328P-AU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NRF24L01" prefix="RF">
<gates>
<gate name="G$1" symbol="NRF24L01"/>
</gates>
<devices>
<device name="" package="NRF24L01">
<connects>
<connect gate="G$1" pin="CE" pad="CE"/>
<connect gate="G$1" pin="CSN" pad="CSN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IRQ" pad="IRQ"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117MP-3.3" prefix="U">
<description>Linear regulators</description>
<gates>
<gate name="A" symbol="LM1117MP-3.3"/>
</gates>
<devices>
<device name="" package="SOT230P696X180-4N">
<connects>
<connect gate="A" pin="ADJ/GND" pad="1"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="A" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LM1117MP-3.3"/>
<attribute name="OC_FARNELL" value="9778195"/>
<attribute name="OC_NEWARK" value="41K3470"/>
<attribute name="PACKAGE" value="SOT223-3"/>
<attribute name="SUPPLIER" value="NationalSemiconductor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P-AU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-AU"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
