<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-11625"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="1k"/>
<element name="R2" library="fab" package="R1206FAB" value="1k"/>
<element name="IC1T44" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
</element>
<element name="XTAL1_20MHZ" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
<element name="R4" library="fab" package="R1206FAB" value="0"/>
<element name="R5" library="fab" package="R1206FAB" value="0"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$2" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="R7" library="fab" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="IC1T44" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="D1" pad="C"/>
<contactref element="S1" pad="1"/>
<contactref element="XTAL1_20MHZ" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="R5" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1T44" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="PA7">
<contactref element="R2" pad="2"/>
<contactref element="IC1T44" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="IC1T44" pad="10"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="PB0">
<contactref element="XTAL1_20MHZ" pad="1"/>
<contactref element="IC1T44" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="IC1T44" pad="3"/>
<contactref element="XTAL1_20MHZ" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="IC1T44" pad="13"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="IC1T44" pad="12"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="IC1T44" pad="7"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="IC1T44" pad="8"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1T44" pad="14"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
<contactref element="IC1T44" pad="9"/>
<contactref element="U$1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
