                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:1363023
Test your 3D printer! v3 by ctrlV is licensed under the Creative Commons - Attribution - No Derivatives license.
http://creativecommons.org/licenses/by-nd/3.0/

# Summary

more Tests in the new **Test your 3D printer! version 3**.   

**new features**  

- Z-Height Check
- Warp Check
- Spike 
- Hole in wall
- Raft Test
- more Overhang Steps 50° - 70° (needs special care, like cooling)
- 2 different extrusion widths: 0.48mm & 0.4mm

This is a hard to print testfile!  
often you don't know if your printer is ready for complex files. with this file you have an easy option to check problematic printing/slicing stuff.  

does your printer challenge this ultimative part?  
check it out and get (almost) instant results.  

these test are included in this very tiny file:

- 01	Nut, Size M4 Nut should fit perfectly
- 02	Wave, rounded print	
- 03	Star,	Sharp Edges	
- 04	Name, Complex Shapes	
- 05	Holes, Size 3, 4, 5 mm
- 06	minimal Distance: 0.1, 0.2, 0.3, 0.4, 0.5, 0.6, 0.7 mm
- 07	Z height: 0.1, 0.2, 0.3, 0.4, 0.5, 0.6, 0.7, 0.8, 0.9, 1.0, 1.1 mm
- 08	Wall Thickness: 0.1, 0.2, 0.3, 0.4, 0.5, 0.6, 0.7 mm
- 09	Bridge Print: 2, 4, 8, 16 mm 
- 10	Sphere, Rounded Print 4.8mm height
- 11	Sphere Mix, 7 mm height
- 12	Pyramide, 7 mm height
- 13	Overhang: 25, 30, 35, 40, 45, 50, 55, 60, 65, 70°
- 14	Warp, does it bend?
- 15	3D Print Font, optimized for 3D printing
- 16	Surface, Flatness
- 17	Size, 100 x 100mm x 23.83 (10mm width)
- 18	Spike, minimum Layer Time, 21 mm height from Bottom (include Baseplate)
- 19	Hole in Wall, 4 mm diameter, check for proper print
- 20	Raft Test, raft should be just under the model
- 21	Retract Travel,	check retract settings for longer travel

version 1 http://www.thingiverse.com/thing:704409
version 2 http://www.thingiverse.com/thing:1019228

check out the forum for more help  
http://www.whoote.com  

# Print Settings

Rafts: Yes
Supports: No
Resolution: 0.1mm or higher
Infill: 30%