<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.3">
<drawing>
<board>
<plain>
<text>satstep@6600</text>
<hole x="3.5" y="60" drill="1.1"/>
<hole x="3.5" y="3.5" drill="1.1"/>
<hole x="51" y="3.5" drill="1.1"/>
<hole x="56.5" y="51.5" drill="1.1"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2512">
</package>
</packages>
</library>
<library name="tb6600hq">
<packages>
<package name="P-HZIP25-1.00G">
</package>
</packages>
</library>
<library name="FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
</packages>
</library>
<library name="Ava">
<packages>
<package name="TS53YL104MR10_TRIMMER">
</package>
</packages>
</library>
<library name="74HC123D">
<packages>
<package name="SOIC127P600X175-16N">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler-2">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="05P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-dil">
<description>&lt;b&gt;DIL Switches and Code Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SD4-05">
<description>&lt;b&gt;DIL/CODE SWITCH&lt;/b&gt;&lt;p&gt;
Mors</description>
</package>
</packages>
</library>
<library name="WEIDMULLER-PM5.08_2_90BLK">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="WEIDMULLER_PM5.08_2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="2512" value="0.68">
<attribute name="PROD_ID" value="RES-12449"/>
</element>
<element name="U$1" library="tb6600hq" package="P-HZIP25-1.00G" value="TB6600HG"/>
<element name="LED" library="FAB_Hello" package="1206" value="GREEN"/>
<element name="R8" library="fab" package="R1206" value="51K"/>
<element name="R9" library="fab" package="R1206" value="1K"/>
<element name="R10" library="fab" package="R1206" value="10K"/>
<element name="C1" library="FAB_Hello" package="1206" value="0.1uF"/>
<element name="C3" library="FAB_Hello" package="1206" value="0.1uF"/>
<element name="C2" library="SparkFun-Capacitors" package="PANASONIC_C" value="100uF"/>
<element name="LED1" library="FAB_Hello" package="1206" value="RED"/>
<element name="R11" library="fab" package="R1206" value="1K"/>
<element name="LED2" library="FAB_Hello" package="1206" value="YELLOW"/>
<element name="C4" library="FAB_Hello" package="1206" value="0.1uF"/>
<element name="C5" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-63V" value="330uF"/>
<element name="C6" library="FAB_Hello" package="1206" value="0.01uF"/>
<element name="R12" library="fab" package="R1206" value="5.1K"/>
<element name="T1" library="Ava" package="TS53YL104MR10_TRIMMER" value="5K"/>
<element name="U1" library="74HC123D" package="SOIC127P600X175-16N" value="74HC123D">
<attribute name="MPN" value="74HC123D"/>
<attribute name="OC_FARNELL" value="1085332"/>
<attribute name="OC_NEWARK" value="99K0580"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="NXP"/>
</element>
<element name="R13" library="fab" package="R1206" value="5.1K"/>
<element name="C7" library="FAB_Hello" package="1206" value="0.1uF"/>
<element name="R14" library="fab" package="R1206" value="499K"/>
<element name="TLP521-1" library="optocoupler" package="DIL04" value=""/>
<element name="4N35" library="optocoupler" package="DIL06" value=""/>
<element name="R15" library="fab" package="R1206" value="330"/>
<element name="R16" library="fab" package="R1206" value="330"/>
<element name="OK1" library="optocoupler-2" package="DIL08" value="6N137"/>
<element name="R17" library="fab" package="R1206" value="330"/>
<element name="R18" library="fab" package="R1206" value="4.7K"/>
<element name="R19" library="fab" package="R1206" value="4.7K"/>
<element name="R20" library="fab" package="R1206" value="4.7K"/>
<element name="R21" library="fab" package="R1206" value="56K"/>
<element name="SW_DIP-5" library="switch-dil" package="SD4-05" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="POWER" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="STEPPER_CONN_1" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="PM5.08/2/90BLK">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="J3" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="STEPPER_CONN_2">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="R22" library="fab" package="R1206" value="1K"/>
<element name="SL1" library="con-amp-quick" package="05P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="ALERT">
<contactref element="U$1" pad="1"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="17"/>
<contactref element="U$1" pad="13"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="R11" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="T1" pad="P$2"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="14"/>
<contactref element="C7" pad="2"/>
<contactref element="TLP521-1" pad="3"/>
<contactref element="TLP521-1" pad="2"/>
<contactref element="4N35" pad="2"/>
<contactref element="OK1" pad="3"/>
<contactref element="4N35" pad="4"/>
<contactref element="OK1" pad="5"/>
<contactref element="R21" pad="2"/>
<contactref element="POWER" pad="1"/>
<contactref element="SL1" pad="5"/>
</signal>
<signal name="LATCH">
<contactref element="U$1" pad="4"/>
<contactref element="SW_DIP-5" pad="9"/>
</signal>
<signal name="1A">
<contactref element="U$1" pad="16"/>
<contactref element="STEPPER_CONN_1" pad="1"/>
</signal>
<signal name="2A">
<contactref element="U$1" pad="14"/>
<contactref element="STEPPER_CONN_1" pad="2"/>
</signal>
<signal name="1B">
<contactref element="U$1" pad="12"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="2B">
<contactref element="U$1" pad="10"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="11"/>
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="U$1" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="T1" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="U$1" pad="21"/>
<contactref element="U1" pad="1"/>
<contactref element="OK1" pad="6"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="DIR">
<contactref element="U$1" pad="22"/>
<contactref element="4N35" pad="5"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="EN">
<contactref element="TLP521-1" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="U$1" pad="18"/>
</signal>
<signal name="M1">
<contactref element="U$1" pad="7"/>
<contactref element="SW_DIP-5" pad="7"/>
</signal>
<signal name="M2">
<contactref element="U$1" pad="8"/>
<contactref element="SW_DIP-5" pad="10"/>
</signal>
<signal name="M3">
<contactref element="U$1" pad="9"/>
<contactref element="SW_DIP-5" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="23"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="24"/>
<contactref element="LED" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="LED2" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="R14" pad="2"/>
<contactref element="OK1" pad="8"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="SW_DIP-5" pad="5"/>
<contactref element="SW_DIP-5" pad="1"/>
<contactref element="SW_DIP-5" pad="2"/>
<contactref element="SW_DIP-5" pad="3"/>
<contactref element="SW_DIP-5" pad="4"/>
<contactref element="LED1" pad="1"/>
<contactref element="SL1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="1"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="19"/>
<contactref element="R10" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R11" pad="2"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="REFAC">
<contactref element="R12" pad="2"/>
<contactref element="T1" pad="P$3"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="13"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="15"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="TLP521-1" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="4N35" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="OK1" pad="2"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="4N35" pad="6"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R16" pad="1"/>
<contactref element="SL1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R15" pad="1"/>
<contactref element="SL1" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="R17" pad="1"/>
<contactref element="SL1" pad="4"/>
</signal>
<signal name="TQ">
<contactref element="U$1" pad="3"/>
<contactref element="SW_DIP-5" pad="6"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$19">
<contactref element="R9" pad="2"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
