<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.38" y2="0" width="0" layer="20"/>
<wire x1="25.38" y1="0" x2="25.38" y2="27.61" width="0" layer="20"/>
<wire x1="25.38" y1="27.61" x2="0" y2="27.61" width="0" layer="20"/>
<wire x1="0" y1="27.61" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R3" library="fab" package="R1206FAB" value="499ohms"/>
<element name="C1" library="fab" package="C1206FAB" value="0.1uf"/>
<element name="DIODE" library="fab" package="SOD123" value=""/>
<element name="N-MOSFET" library="fab" package="SOT-23" value=""/>
<element name="GATE-RES" library="fab" package="R1206FAB" value="100"/>
<element name="PULL-UP-RES" library="fab" package="R1206FAB" value="1K"/>
<element name="CONNECTOR-MOTOR" library="SparkFun-Connectors" package="1X02_LONGPADS" value=""/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
</elements>
<signals>
<signal name="GND">
<contactref element="N-MOSFET" pad="2"/>
<contactref element="PULL-UP-RES" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="DIODE" pad="CATHODE"/>
<contactref element="C1" pad="2"/>
<contactref element="CONNECTOR-MOTOR" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="N-MOSFET" pad="1"/>
<contactref element="DIODE" pad="ANODE"/>
<contactref element="CONNECTOR-MOTOR" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VIB">
<contactref element="GATE-RES" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="GATE-RES" pad="2"/>
<contactref element="PULL-UP-RES" pad="2"/>
<contactref element="N-MOSFET" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="LED">
<contactref element="U$1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
