<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="2X02SMD">
</package>
</packages>
<symbols>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="V_REG_LM1117" prefix="U" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-08170"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="VREG3.3V" library="fab" deviceset="V_REG_LM1117" device="SOT223"/>
<part name="C1" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="1uF"/>
<part name="IN-5V" library="fab" deviceset="FTDI-SMD-HEADER" device=""/>
<part name="C2" library="fab" deviceset="CAP-UNPOLARIZED" device="FAB" value="10uF"/>
<part name="OUT-3.3V" library="fab" deviceset="PINHD-2X2-SMD" device=""/>
</parts>
<sheets>
<sheet>
<plain>
<text>OUT 3.3V power supply</text>
<text>IN 5V power supply</text>
</plain>
<busses>
</busses>
<nets>
<net name="CTS">
<segment>
<pinref part="IN-5V" gate="G$1" pin="CTS"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="IN-5V" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="IN-5V" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="RTS">
<segment>
<pinref part="IN-5V" gate="G$1" pin="RTS"/>
</segment>
</net>
<net name="GND-OUT">
<segment>
<pinref part="C1" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="OUT-3.3V" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="OUT-3.3V" gate="G$1" pin="4"/>
</segment>
<segment>
<pinref part="C2" gate="&gt;NAME" pin="2"/>
</segment>
<segment>
<pinref part="VREG3.3V" gate="G$1" pin="ADJ"/>
</segment>
<segment>
<pinref part="IN-5V" gate="G$1" pin="GND"/>
</segment>
</net>
<net name="VCC-IN">
<segment>
<pinref part="C2" gate="&gt;NAME" pin="1"/>
</segment>
<segment>
<pinref part="IN-5V" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="VREG3.3V" gate="G$1" pin="IN"/>
</segment>
</net>
<net name="VCC-OUT">
<segment>
<pinref part="OUT-3.3V" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="OUT-3.3V" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="VREG3.3V" gate="G$1" pin="OUT"/>
</segment>
<segment>
<pinref part="VREG3.3V" gate="G$1" pin="OUT@1"/>
</segment>
<segment>
<pinref part="C1" gate="&gt;NAME" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
