<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="fab">
<packages>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="R1206FAB">
</package>
</packages>
<symbols>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="BC" library="fab" deviceset="LED" device="FAB1206"/>
<part name="CD" library="fab" deviceset="LED" device="FAB1206"/>
<part name="BA" library="fab" deviceset="LED" device="FAB1206"/>
<part name="CB" library="fab" deviceset="LED" device="FAB1206"/>
<part name="DE" library="fab" deviceset="LED" device="FAB1206"/>
<part name="DB" library="fab" deviceset="LED" device="FAB1206"/>
<part name="BD" library="fab" deviceset="LED" device="FAB1206"/>
<part name="DC" library="fab" deviceset="LED" device="FAB1206"/>
<part name="AC" library="fab" deviceset="LED" device="FAB1206"/>
<part name="ED" library="fab" deviceset="LED" device="FAB1206"/>
<part name="AB" library="fab" deviceset="LED" device="FAB1206"/>
<part name="B" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="A" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="C" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="D" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="E" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R1" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R2" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R3" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R4" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R5" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R6" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R7" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R8" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R9" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="EB" library="fab" deviceset="LED" device="FAB1206"/>
<part name="CA" library="fab" deviceset="LED" device="FAB1206"/>
<part name="BE" library="fab" deviceset="LED" device="FAB1206"/>
<part name="EC" library="fab" deviceset="LED" device="FAB1206"/>
<part name="CE" library="fab" deviceset="LED" device="FAB1206"/>
<part name="R10" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R12" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="R14" library="fab" deviceset="RES-US" device="1206FAB"/>
<part name="JP1" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP2" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP3" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP4" library="pinhead" deviceset="PINHD-1X1" device=""/>
<part name="JP5" library="pinhead" deviceset="PINHD-1X1" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="A">
<segment>
<pinref part="A" gate="G$1" pin="2"/>
<pinref part="AB" gate="G$1" pin="A"/>
<pinref part="BA" gate="G$1" pin="C"/>
<pinref part="AC" gate="G$1" pin="A"/>
<pinref part="CA" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="AB" gate="G$1" pin="C"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="BC" gate="G$1" pin="C"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="D">
<segment>
<pinref part="CD" gate="G$1" pin="C"/>
<pinref part="D" gate="G$1" pin="2"/>
<pinref part="DE" gate="G$1" pin="A"/>
<pinref part="R8" gate="G$1" pin="2"/>
<pinref part="R9" gate="G$1" pin="1"/>
<pinref part="DB" gate="G$1" pin="A"/>
<pinref part="ED" gate="G$1" pin="C"/>
</segment>
</net>
<net name="E">
<segment>
<pinref part="E" gate="G$1" pin="2"/>
<pinref part="DE" gate="G$1" pin="C"/>
<pinref part="R10" gate="G$1" pin="1"/>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="BE" gate="G$1" pin="C"/>
<pinref part="EB" gate="G$1" pin="A"/>
<pinref part="ED" gate="G$1" pin="A"/>
</segment>
</net>
<net name="B">
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
<pinref part="B" gate="G$1" pin="2"/>
<pinref part="BC" gate="G$1" pin="A"/>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="CB" gate="G$1" pin="C"/>
<pinref part="BD" gate="G$1" pin="A"/>
<pinref part="DB" gate="G$1" pin="C"/>
<pinref part="R12" gate="G$1" pin="2"/>
<pinref part="R14" gate="G$1" pin="2"/>
</segment>
</net>
<net name="C">
<segment>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="C" gate="G$1" pin="2"/>
<pinref part="CD" gate="G$1" pin="A"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="DC" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="1"/>
<pinref part="R7" gate="G$1" pin="1"/>
<pinref part="CE" gate="G$1" pin="A"/>
<pinref part="EC" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="BA" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="CB" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="DC" gate="G$1" pin="A"/>
<pinref part="R8" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="R9" gate="G$1" pin="2"/>
<pinref part="BD" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="AC" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="CA" gate="G$1" pin="A"/>
<pinref part="R7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="CE" gate="G$1" pin="C"/>
<pinref part="R10" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="EC" gate="G$1" pin="A"/>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="R12" gate="G$1" pin="1"/>
<pinref part="BE" gate="G$1" pin="A"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="R14" gate="G$1" pin="1"/>
<pinref part="EB" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="JP1" gate="G$1" pin="1"/>
<pinref part="A" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="JP2" gate="G$1" pin="1"/>
<pinref part="B" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$15">
<segment>
<pinref part="JP3" gate="G$1" pin="1"/>
<pinref part="C" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$16">
<segment>
<pinref part="JP4" gate="G$1" pin="1"/>
<pinref part="D" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="JP5" gate="G$1" pin="1"/>
<pinref part="E" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
