<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="4.318" y1="11.938" x2="77.902" y2="12.192" width="0" layer="20"/>
<wire x1="77.902" y1="12.192" x2="75.616" y2="69.332" width="0" layer="20"/>
<wire x1="75.616" y1="69.332" x2="4.572" y2="69.078" width="0" layer="20"/>
<wire x1="4.572" y1="69.078" x2="4.318" y2="11.938" width="0" layer="20"/>
<text>BUGGY LEDS</text>
<polygon width="0.3048" layer="46">
<vertex x="19.304" y="61.214"/>
<vertex x="9.906" y="51.816"/>
<vertex x="9.906" y="37.592"/>
<vertex x="9.906" y="36.576"/>
<vertex x="22.606" y="23.876"/>
<vertex x="57.658" y="23.876"/>
<vertex x="74.422" y="40.64"/>
<vertex x="74.422" y="50.546"/>
<vertex x="64.008" y="60.96"/>
<vertex x="63.754" y="61.214"/>
<vertex x="19.05" y="61.214"/>
</polygon>
</plain>
<libraries>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON-6.8MM">
<description>Part#: MS621FE-FL11E</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD">
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="_hhn_78xx_79xx_NCV78xx_d2pak_dpak">
<description>&lt;h2&gt;78xx 79xx NCV78xx SMD (D2PAK, DPAK)&lt;/h2&gt;
&lt;p&gt;&lt;b&gt;Linear Voltage Regulators&lt;/b&gt;&lt;/p&gt;
Source: ONSEMI (http://onsemi.com)&lt;br /&gt;
&lt;hr&gt;
&lt;p&gt;&lt;i&gt;Author: Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn, rainer.bayer@hs-heilbronn.de&lt;br /&gt;
Ingenieurbüro ing-rb, mail@ing-rb.de&lt;/p&gt;</description>
<packages>
<package name="DPAK-3">
<description>&lt;b&gt;DPAK-3&lt;/b&gt; (acc. to. ON Semiconductor specs)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BT1" library="SparkFun-Batteries" package="BATTCON-6.8MM" value="6.8MM_COIN_CELL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-13734"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="_hhn_78xx_79xx_NCV78xx_d2pak_dpak" package="DPAK-3" value="MC78GENERICDT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="U1" pad="4"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="BT1" pad="-"/>
<contactref element="U$1" pad="6"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="9V">
<contactref element="U1" pad="1"/>
<contactref element="BT1" pad="+"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="BUTTON">
<contactref element="IC1" pad="3"/>
<contactref element="S1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
