<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<schematic>
<libraries>
<library name="atmega8">
<packages>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
<symbols>
<symbol name="ATMEGA48/88/168-TQFP/QFN32">
<pin name="PB5(SCK/PCINT5)"/>
<pin name="PB7(XTAL2/TOSC2/PCINT7)"/>
<pin name="PB6(XTAL1/TOSC1/PCINT6)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pas"/>
<pin name="PB4(MISO/PCINT4)"/>
<pin name="PB3(MOSI/OC2A/PCINT3)"/>
<pin name="PB2(SS/OC1B/PCINT2)"/>
<pin name="PB1(OC1A/PCINT1)"/>
<pin name="PB0(ICP1/CLKO/PCINT0)"/>
<pin name="PD7(AIN1/PCINT23)"/>
<pin name="PD6(AIN0/OC0A/PCINT22)"/>
<pin name="PD5(T1/OC0B/PCINT21)"/>
<pin name="PD4(T0/XCK/PCINT20)"/>
<pin name="PD3(INT1/OC2B/PCINT19)"/>
<pin name="PD2(INT0/PCINT18)"/>
<pin name="PD1(TXD/PCINT17)"/>
<pin name="PD0(RXD/PCINT16)"/>
<pin name="PC5(ADC5/SCL/PCINT13)"/>
<pin name="PC4(ADC4/SDA/PCINT12)"/>
<pin name="PC3(ADC3/PCINT11)"/>
<pin name="PC2(ADC2/PCINT10)"/>
<pin name="PC1(ADC1/PCINT9)"/>
<pin name="PC0(ADC0/PCINT8)"/>
<pin name="PC6(/RESET/PCINT14)"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="ADC7" direction="pas"/>
<pin name="ADC6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA48/88/168" prefix="IC">
<gates>
<gate name="1" symbol="ATMEGA48/88/168-TQFP/QFN32"/>
</gates>
<devices>
<device name="-MU" package="MLF32">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AU" package="TQFP32-08">
<connects>
<connect gate="1" pin="ADC6" pad="19"/>
<connect gate="1" pin="ADC7" pad="22"/>
<connect gate="1" pin="AGND" pad="21"/>
<connect gate="1" pin="AREF" pad="20"/>
<connect gate="1" pin="AVCC" pad="18"/>
<connect gate="1" pin="GND@1" pad="3"/>
<connect gate="1" pin="GND@2" pad="5"/>
<connect gate="1" pin="PB0(ICP1/CLKO/PCINT0)" pad="12"/>
<connect gate="1" pin="PB1(OC1A/PCINT1)" pad="13"/>
<connect gate="1" pin="PB2(SS/OC1B/PCINT2)" pad="14"/>
<connect gate="1" pin="PB3(MOSI/OC2A/PCINT3)" pad="15"/>
<connect gate="1" pin="PB4(MISO/PCINT4)" pad="16"/>
<connect gate="1" pin="PB5(SCK/PCINT5)" pad="17"/>
<connect gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)" pad="7"/>
<connect gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)" pad="8"/>
<connect gate="1" pin="PC0(ADC0/PCINT8)" pad="23"/>
<connect gate="1" pin="PC1(ADC1/PCINT9)" pad="24"/>
<connect gate="1" pin="PC2(ADC2/PCINT10)" pad="25"/>
<connect gate="1" pin="PC3(ADC3/PCINT11)" pad="26"/>
<connect gate="1" pin="PC4(ADC4/SDA/PCINT12)" pad="27"/>
<connect gate="1" pin="PC5(ADC5/SCL/PCINT13)" pad="28"/>
<connect gate="1" pin="PC6(/RESET/PCINT14)" pad="29"/>
<connect gate="1" pin="PD0(RXD/PCINT16)" pad="30"/>
<connect gate="1" pin="PD1(TXD/PCINT17)" pad="31"/>
<connect gate="1" pin="PD2(INT0/PCINT18)" pad="32"/>
<connect gate="1" pin="PD3(INT1/OC2B/PCINT19)" pad="1"/>
<connect gate="1" pin="PD4(T0/XCK/PCINT20)" pad="2"/>
<connect gate="1" pin="PD5(T1/OC0B/PCINT21)" pad="9"/>
<connect gate="1" pin="PD6(AIN0/OC0A/PCINT22)" pad="10"/>
<connect gate="1" pin="PD7(AIN1/PCINT23)" pad="11"/>
<connect gate="1" pin="VCC@1" pad="4"/>
<connect gate="1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<packages>
</packages>
<symbols>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="5MM">
<description>5 mm, round</description>
</package>
<package name="0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="AVX_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/04/2012 16:26:10</description>
<packages>
<package name="CAPC3216X178N">
</package>
</packages>
<symbols>
<symbol name="CAPH">
<pin name="C2" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="0612ZC225MAT2A" prefix="C">
<description>Capacitor 1206</description>
<gates>
<gate name="A" symbol="CAPH"/>
</gates>
<devices>
<device name="" package="CAPC3216X178N">
<connects>
<connect gate="A" pin="C1" pad="1"/>
<connect gate="A" pin="C2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="0612ZC225MAT2A"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="12N3209"/>
<attribute name="SUPPLIER" value="AVX"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VALUE" value="2.2µF"/>
<attribute name="VOLTAGERATING" value="10V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="AXIAL-0.3">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="GRM43D">
</package>
<package name="0603-CAP">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="AXIAL-5MM">
</package>
<package name="1210">
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH 1/10th watt (small) resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-CAP" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-CAP" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="L7805">
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="L7805" prefix="IC">
<description>ICP001</description>
<gates>
<gate name="1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXS">
<connects>
<connect gate="1" pin="GND" pad="GND"/>
<connect gate="1" pin="IN" pad="IN"/>
<connect gate="1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MP" value="L7805"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-ptr500">
<description>&lt;b&gt;PTR Connectors&lt;/b&gt;&lt;p&gt;
Aug. 2004 / PTR Meßtechnik:&lt;br&gt;
Die Bezeichnung der Serie AK505 wurde geändert.&lt;br&gt;
Es handelt sich hierbei um AK500 in horizontaler Ausführung.&lt;p&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Alte Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Neue Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2DS,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2DS-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AKZ505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AKZ500/2-5.08-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TABLE&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AK300/2">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="KL">
<pin name="KL" direction="pas"/>
</symbol>
<symbol name="KLV">
<pin name="KL" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AK300/2" prefix="X" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="-1" symbol="KL"/>
<gate name="-2" symbol="KLV"/>
</gates>
<devices>
<device name="" package="AK300/2">
<connects>
<connect gate="-1" pin="KL" pad="1"/>
<connect gate="-2" pin="KL" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2031">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232031_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="22-23-2041">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 4 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232041_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="22-23-2031" prefix="X">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
</gates>
<devices>
<device name="" package="22-23-2031">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-23-2041" prefix="X">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="" package="22-23-2041">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="OC_FARNELL" value="1462920"/>
<attribute name="OC_NEWARK" value="38C0355"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="CT3216">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 reflow solder&lt;/b&gt;&lt;p&gt;KEMET S / EIA 3216-12</description>
</package>
<package name="A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 reflow solder&lt;/b&gt;&lt;p&gt;KEMET T / EIA 3528-12</description>
</package>
<package name="B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 reflow solder&lt;/b&gt;&lt;p&gt;KEMET U / EIA 6032-15</description>
</package>
<package name="C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 reflow solder</description>
</package>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 reflow solder&lt;/b&gt;</description>
</package>
<package name="E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 reflow solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_Z">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_P">
<description>&lt;b&gt;Chip Capacitor&lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_B">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SANYO-OSCON_9E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_9F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_A">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_A'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_B'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_D">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E1">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_E9">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F'">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F0">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F13">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_G">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_H">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt;&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_A5">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_B6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_C6">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_E7">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F12">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="SANYO-OSCON_SMD_F8">
<description>&lt;b&gt;SANYO OSCON Capacitor&lt;/b&gt; SMD type with conductive polymer electrolyte&lt;p&gt;
Source: e_os_all.pdf</description>
</package>
<package name="UD-10X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 10 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-4X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 4 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-5X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 5 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-6,3X5,8_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 5.8 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-6,3X7,7_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 6.3 x 7.7 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
<package name="UD-8X10_NICHICON">
<description>&lt;b&gt;ALUMINUM ELECTROLYTIC CAPACITORS&lt;/b&gt; UD Series 8 x 10 mm&lt;p&gt;
Source: http://products.nichicon.co.jp/en/pdf/XJA043/e-ud.pdf</description>
</package>
</packages>
<symbols>
<symbol name="CPOL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CPOL-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="CPOL"/>
</gates>
<devices>
<device name="CT3216" package="CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT3528" package="CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT6032" package="CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="CT7343" package="CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181A" package="B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181B" package="B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181C" package="B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B45181D" package="B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D4" package="TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D4L" package="TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D5" package="TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D6" package="TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D6L" package="TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D7L" package="TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D7" package="TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D10" package="TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D11" package="TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D11L" package="TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT6D6" package="TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D6L" package="TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D7" package="TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D7L" package="TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D9" package="TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT5D9L" package="TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR1" package="ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR2" package="ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR3" package="ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR4" package="ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="ETR5" package="ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-35" package="P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-40" package="P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-50" package="P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="P128-60" package="P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-45" package="TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-50" package="TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-70" package="TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-60" package="TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TAP5-80" package="TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E1.8-4" package="E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-5AXIAL" package="E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-6AXIAL" package="E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E15-9AXIAL" package="E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-5V" package="E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-5" package="E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-6" package="E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-7" package="E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2.5-4V" package="E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2-4" package="E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2-5" package="E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-10AXIAL" package="E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-6AXIAL" package="E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E22-9AXIAL" package="E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E3.5-10" package="E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E25-10AXIAL" package="E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E25-9AXIAL" package="E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E3.5-8" package="E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-10AXIAL" package="E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-12AXIAL" package="E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E30-16AXIAL" package="E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-12AXIAL" package="E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-14AXIAL" package="E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-16AXIAL" package="E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E35-18AXIAL" package="E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-16AXIAL" package="E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-18AXIAL" package="E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-21AXIAL" package="E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-22AXIAL" package="E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E45-25AXIAL" package="E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-10.5" package="E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-13" package="E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-4" package="E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-5" package="E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-6" package="E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-8.5" package="E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E50-25AXIAL" package="E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E50-30AXIAL" package="E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E55-25AXIAL" package="E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E55-30AXIAL" package="E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E5-9VAXIAL" package="E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E7.5-16" package="E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E7.5-18" package="E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-20" package="EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-22.5" package="EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-25" package="EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-30" package="EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E10-35" package="EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1R" package="085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1W" package="085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1AR" package="085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="085CS-1AW" package="085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-2R" package="139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-2W" package="139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-3R" package="139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="139CLL-3W" package="139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-0810" package="140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-1010" package="140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="140CLH-1014" package="140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-0810" package="150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-1010" package="150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="150CLZ-1014" package="150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0405" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0505" package="153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0605" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0807" package="153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-0810" package="153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1010" package="153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1012" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="153CLV-1014" package="153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="175TMP-0808" package="175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="175TMP-0810" package="175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A/3216-18R" package="A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A/3216-18W" package="A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B/3528-21R" package="B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B/3528-21W" package="B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C/6032-28R" package="C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C/6032-28W" package="C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D/7343-31R" package="D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D/7343-31W" package="D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E/7260-38R" package="E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E/7260-38W" package="E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="R/2012-12R" package="R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="R/2012-12W" package="R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="A" package="PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="B" package="PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="F" package="PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="TT2D5L" package="TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="E2,5-6E" package="E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCA" package="SMC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCZ" package="SMC_Z">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCP" package="SMC_P">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCB" package="SMC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCC" package="SMC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCD" package="SMC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SMCE" package="SMC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_9E" package="SANYO-OSCON_9E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_9F" package="SANYO-OSCON_9F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_A" package="SANYO-OSCON_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_A'" package="SANYO-OSCON_A'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_B" package="SANYO-OSCON_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_B'" package="SANYO-OSCON_B'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C" package="SANYO-OSCON_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C'" package="SANYO-OSCON_C'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_C6" package="SANYO-OSCON_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_D" package="SANYO-OSCON_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E" package="SANYO-OSCON_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E'" package="SANYO-OSCON_E'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E1" package="SANYO-OSCON_E1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E12" package="SANYO-OSCON_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E13" package="SANYO-OSCON_E13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E7" package="SANYO-OSCON_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_E9" package="SANYO-OSCON_E9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F" package="SANYO-OSCON_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F'" package="SANYO-OSCON_F'">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F0" package="SANYO-OSCON_F0">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F13" package="SANYO-OSCON_F13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_F8" package="SANYO-OSCON_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_G" package="SANYO-OSCON_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_H" package="SANYO-OSCON_H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_A5" package="SANYO-OSCON_SMD_A5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_B6" package="SANYO-OSCON_SMD_B6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_C6" package="SANYO-OSCON_SMD_C6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_E12" package="SANYO-OSCON_SMD_E12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_E7" package="SANYO-OSCON_SMD_E7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_F12" package="SANYO-OSCON_SMD_F12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="SANYO_SMD_F8" package="SANYO-OSCON_SMD_F8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-10X10" package="UD-10X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-4X5,8" package="UD-4X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-5X5,8" package="UD-5X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-6,3X8,8" package="UD-6,3X5,8_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-6,3X7,7" package="UD-6,3X7,7_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
<device name="UD-8X10" package="UD-8X10_NICHICON">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SPICEPREFIX" value="C"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fab">
<packages>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
high speed (Philips)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="78XXS" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXS">
<connects>
<connect gate="1" pin="GND" pad="GND"/>
<connect gate="1" pin="IN" pad="IN"/>
<connect gate="1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="ABM3-8.000MHZ-D2Y-T">
<packages>
<package name="XTAL500X320X130N">
</package>
</packages>
<symbols>
<symbol name="ABM3-8.000MHZ-D2Y-T">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ABM3-8.000MHZ-D2Y-T" prefix="Y">
<description>Crystals 12MHz 18pF 30ppm -40C +85C</description>
<gates>
<gate name="G$1" symbol="ABM3-8.000MHZ-D2Y-T"/>
</gates>
<devices>
<device name="" package="XTAL500X320X130N">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Crystal 8MHz Ø·Â¢Ø¢Â±20ppm _Tol_ Ø·Â¢Ø¢Â±30ppm _Stability_ 18pF FUND 500Ohm 2-Pin CSMD T/R  "/>
<attribute name="MF" value="Abracon"/>
<attribute name="MP" value="ABM3-8.000MHZ-D2Y-T"/>
<attribute name="PACKAGE" value="SMD-2 Abracon"/>
<attribute name="PRICE" value="None"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="myFab">
<packages>
<package name="2X3PINHEADER">
</package>
</packages>
<symbols>
<symbol name="2X3PINHEADER">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2X3PINHEADER" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2X3PINHEADER"/>
</gates>
<devices>
<device name="" package="2X3PINHEADER">
<connects>
<connect gate="A" pin="1" pad="GND"/>
<connect gate="A" pin="2" pad="RST"/>
<connect gate="A" pin="3" pad="MOSI"/>
<connect gate="A" pin="4" pad="SCK"/>
<connect gate="A" pin="5" pad="VCC"/>
<connect gate="A" pin="6" pad="MISO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="1X06M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
<package name="1X06SMD">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 SMD</description>
</package>
<package name="1X06SMD/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
</packages>
<symbols>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="_2.54" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-90°" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.00" package="1X06M">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD" package="1X06SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.54-SMD-90°" package="1X06SMD/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="heatsink-jonathan">
<description>&lt;b&gt;Heatsinks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SK104-PAD">
<description>&lt;b&gt;HEATSINK&lt;/b&gt;&lt;p&gt; manufacturer Fischer/distributor Buerklin</description>
</package>
</packages>
<symbols>
<symbol name="KK-2">
<pin name="K@1" direction="pas"/>
<pin name="K@2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SK104-PAD" prefix="KK">
<description>&lt;b&gt;HEATSINK&lt;/b&gt;&lt;p&gt; manufacturer Fischer/distributor Buerklin</description>
<gates>
<gate name="G$1" symbol="KK-2"/>
</gates>
<devices>
<device name="" package="SK104-PAD">
<connects>
<connect gate="G$1" pin="K@1" pad="K1"/>
<connect gate="G$1" pin="K@2" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DPAK">
</package>
<package name="SOT323">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
<package name="TO-263/D2PAK">
</package>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
<symbols>
<symbol name="LABELED-NMOS">
<description>&lt;h3&gt; N-channel MOSFET transistor&lt;/h3&gt;
Switches electronic signals</description>
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MOSFET-NCH" prefix="Q">
<description>&lt;h3&gt;N-channel MOSFETs&lt;/h3&gt;
&lt;p&gt;Voltage controlled devices that allow control of high current outputs.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13261”&gt;SparkFun OpenScale&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12651”&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10182”&gt;SparkFun Monster Moto Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11214”&gt;SparkFun MOSFET Power Controller&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="NMOS" symbol="LABELED-NMOS"/>
</gates>
<devices>
<device name="-FDD8780" package="DPAK">
<connects>
<connect gate="NMOS" pin="D" pad="4"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="VALUE" value="35A/25V/8.5mΩ"/>
</technology>
</technologies>
</device>
<device name="-2N7002PW" package="SOT323">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE" value="310mA/60V/1.6Ω"/>
</technology>
</technologies>
</device>
<device name="-FQP30N06L" package="TO220V">
<connects>
<connect gate="NMOS" pin="D" pad="2"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="VALUE" value="60V/32A/35mΩ"/>
</technology>
</technologies>
</device>
<device name="-BSS138" package="SOT23-3">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE" value="220mA/50V/3.5Ω"/>
</technology>
</technologies>
</device>
<device name="-PSMN7R0" package="TO-263/D2PAK">
<connects>
<connect gate="NMOS" pin="D" pad="2"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12437"/>
<attribute name="VALUE" value="100A/100V/6.8mΩ"/>
</technology>
</technologies>
</device>
<device name="-AO3404A" package="SOT23-3">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12988"/>
<attribute name="VALUE" value="5.8A/30V/35mΩ"/>
</technology>
</technologies>
</device>
<device name="-FDS6630A" package="SO08">
<connects>
<connect gate="NMOS" pin="D" pad="5 6 7 8"/>
<connect gate="NMOS" pin="G" pad="4"/>
<connect gate="NMOS" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08089"/>
<attribute name="VALUE" value="6.5A/30V/38mΩ"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="MICRO" library="atmega8" deviceset="ATMEGA48/88/168" device="-AU" value="ATMEGA328P"/>
<part name="P+7" library="supply1" deviceset="VCC" device=""/>
<part name="C1" library="AVX_By_element14_Batch_1" deviceset="0612ZC225MAT2A" device="" value="22pF"/>
<part name="C2" library="AVX_By_element14_Batch_1" deviceset="0612ZC225MAT2A" device="" value="22pF"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="R1" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="SWITCH" library="01_FAB_Hello" deviceset="6MM_SWITCH" device="6MM_SWITCH"/>
<part name="LED_13" library="01_FAB_Hello" deviceset="LED" device="1206" value="YELLOW"/>
<part name="LED_GREEN" library="01_FAB_Hello" deviceset="LED" device="1206"/>
<part name="R2" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="499"/>
<part name="R3" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="499"/>
<part name="C3" library="01_SparkFun" deviceset="CAP" device="1206" value="10uF"/>
<part name="C4" library="01_SparkFun" deviceset="CAP" device="1206" value="1uF"/>
<part name="C5" library="01_SparkFun" deviceset="CAP" device="1206" value="100nF"/>
<part name="C6" library="01_SparkFun" deviceset="CAP" device="1206" value="100nF"/>
<part name="IC1" library="L7805" deviceset="L7805" device=""/>
<part name="+--R" library="con-ptr500" deviceset="AK300/2" device=""/>
<part name="MOTOR1" library="con-molex" deviceset="22-23-2031" device=""/>
<part name="MOTOR2" library="con-molex" deviceset="22-23-2031" device=""/>
<part name="HM-10" library="con-molex" deviceset="22-23-2041" device=""/>
<part name="C14" library="rcl" deviceset="CPOL-EU" device="E2.5-6" value="470UF/25V"/>
<part name="C23" library="rcl" deviceset="CPOL-EU" device="E2.5-6" value="47UF/15"/>
<part name="C13" library="rcl" deviceset="CPOL-EU" device="E2.5-6" value="47UF"/>
<part name="C12" library="rcl" deviceset="CPOL-EU" device="E2.5-6" value="470UF/25V"/>
<part name="ZENER-LEVEL" library="fab" deviceset="DIODE" device="SOD123"/>
<part name="R-FSR1" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R-FSR2" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R1-LED" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R1-LEVEL" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="100k"/>
<part name="R2-LEVEL" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="5k"/>
<part name="R2-LED" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="R3-LED" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="10k"/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="GND15" library="supply1" deviceset="GND" device=""/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
<part name="GND17" library="supply1" deviceset="GND" device=""/>
<part name="FSR-2" library="con-ptr500" deviceset="AK300/2" device=""/>
<part name="FSR-1" library="con-ptr500" deviceset="AK300/2" device=""/>
<part name="G--B" library="con-ptr500" deviceset="AK300/2" device=""/>
<part name="+--GND" library="con-ptr500" deviceset="AK300/2" device=""/>
<part name="R1-LED1" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="100"/>
<part name="R1-LED2" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="100"/>
<part name="R1-LED3" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="100"/>
<part name="IC2" library="v-reg" deviceset="78XXS" device=""/>
<part name="CRYSTAL" library="ABM3-8.000MHZ-D2Y-T" deviceset="ABM3-8.000MHZ-D2Y-T" device="" value="16Mhz"/>
<part name="SPI" library="myFab" deviceset="2X3PINHEADER" device=""/>
<part name="FTDI" library="pinhead-1" deviceset="PINHD-1X6" device="_2.54-SMD-90°" value="FTDI"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="R4" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="2000"/>
<part name="R5" library="01_SparkFun" deviceset="RESISTOR" device="1206" value="1000"/>
<part name="GND18" library="supply1" deviceset="GND" device=""/>
<part name="HEATSINKL7805" library="heatsink-jonathan" deviceset="SK104-PAD" device=""/>
<part name="HEATSINKL7812" library="heatsink-jonathan" deviceset="SK104-PAD" device=""/>
<part name="MOSFET-LED1" library="SparkFun-DiscreteSemi" deviceset="MOSFET-NCH" device="-PSMN7R0" value="IRFZ44N"/>
<part name="MOSFET-LED2" library="SparkFun-DiscreteSemi" deviceset="MOSFET-NCH" device="-PSMN7R0" value="IRFZ44N"/>
<part name="MOSFET-LED3" library="SparkFun-DiscreteSemi" deviceset="MOSFET-NCH" device="-PSMN7R0" value="IRFZ44N"/>
</parts>
<sheets>
<sheet>
<plain>
<text>LED CIRCUIT</text>
<text>FSR CIRCUIT</text>
<text>MOTOR CIRCUIT (PWM)</text>
<text>HM-10 (BLUETOOTH)</text>
<text>Batterie Level Circuit</text>
<text>12V CIRCUIT</text>
<text>5V CIRCUIT</text>
<text>INPUT FILTER</text>
<text>ATMEL 328P CIRCUIT (SMD)</text>
<text>SPI INTERFACE</text>
<text>FTDI INTERFACE</text>
</plain>
<busses>
</busses>
<nets>
<net name="VCC">
<segment>
<pinref part="MICRO" gate="1" pin="VCC@1"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="VCC@2"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="AVCC"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="AREF"/>
</segment>
<segment>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="LED_GREEN" gate="G$1" pin="A"/>
<pinref part="IC1" gate="1" pin="OUT"/>
<pinref part="C23" gate="G$1" pin="+"/>
</segment>
<segment>
<pinref part="P+7" gate="VCC" pin="VCC"/>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="C5" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="FSR-1" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="FSR-2" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="HM-10" gate="-1" pin="S"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="5"/>
<pinref part="P+1" gate="VCC" pin="VCC"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="C4" gate="G$1" pin="2"/>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="GND@1"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="GND@2"/>
</segment>
<segment>
<pinref part="C1" gate="A" pin="C1"/>
</segment>
<segment>
<pinref part="C2" gate="A" pin="C1"/>
</segment>
<segment>
<pinref part="SWITCH" gate="2" pin="S"/>
<pinref part="SWITCH" gate="2" pin="S1"/>
</segment>
<segment>
<pinref part="MICRO" gate="1" pin="AGND"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="MOTOR1" gate="-3" pin="S"/>
</segment>
<segment>
<pinref part="R-FSR2" gate="G$1" pin="2"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R-FSR1" gate="G$1" pin="2"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R1-LED" gate="G$1" pin="1"/>
<pinref part="GND13" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="MOSFET-LED1" gate="NMOS" pin="S"/>
</segment>
<segment>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="R2-LED" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="GND4" gate="1" pin="GND"/>
<pinref part="MOSFET-LED2" gate="NMOS" pin="S"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="MOSFET-LED3" gate="NMOS" pin="S"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="R3-LED" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="HM-10" gate="-2" pin="S"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R2-LEVEL" gate="G$1" pin="2"/>
<pinref part="GND15" gate="1" pin="GND"/>
<pinref part="ZENER-LEVEL" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="GND17" gate="1" pin="GND"/>
<pinref part="C12" gate="G$1" pin="-"/>
<pinref part="C13" gate="G$1" pin="-"/>
<pinref part="IC2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C23" gate="G$1" pin="-"/>
<pinref part="GND16" gate="1" pin="GND"/>
<pinref part="C14" gate="G$1" pin="-"/>
<pinref part="IC1" gate="1" pin="GND"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="+--GND" gate="-2" pin="KL"/>
</segment>
<segment>
<pinref part="MOTOR2" gate="-3" pin="S"/>
<pinref part="GND12" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="1"/>
<pinref part="GND2" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="FTDI" gate="A" pin="1"/>
<pinref part="GND14" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="GND18" gate="1" pin="GND"/>
</segment>
</net>
<net name="N$12">
<segment>
<pinref part="MICRO" gate="1" pin="PB5(SCK/PCINT5)"/>
<pinref part="LED_13" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="4"/>
</segment>
</net>
<net name="N$26">
<segment>
<pinref part="LED_GREEN" gate="G$1" pin="C"/>
<pinref part="R2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$27">
<segment>
<pinref part="LED_13" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="RESET-FTDI">
<segment>
<pinref part="C6" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="FTDI" gate="A" pin="6"/>
</segment>
</net>
<net name="N$29">
<segment>
<pinref part="G--B" gate="-1" pin="KL"/>
<pinref part="MOSFET-LED1" gate="NMOS" pin="D"/>
</segment>
</net>
<net name="N$30">
<segment>
<pinref part="G--B" gate="-2" pin="KL"/>
<pinref part="MOSFET-LED2" gate="NMOS" pin="D"/>
</segment>
</net>
<net name="N$31">
<segment>
<pinref part="+--R" gate="-1" pin="KL"/>
<pinref part="MOSFET-LED3" gate="NMOS" pin="D"/>
</segment>
</net>
<net name="LED1-PWM">
<segment>
<pinref part="MICRO" gate="1" pin="PB1(OC1A/PCINT1)"/>
</segment>
<segment>
<pinref part="R1-LED1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="LED2-PWM">
<segment>
<pinref part="MICRO" gate="1" pin="PB2(SS/OC1B/PCINT2)"/>
</segment>
<segment>
<pinref part="R1-LED2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="LED3-PWM">
<segment>
<pinref part="MICRO" gate="1" pin="PB3(MOSI/OC2A/PCINT3)"/>
</segment>
<segment>
<pinref part="R1-LED3" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="3"/>
</segment>
</net>
<net name="N$7">
<segment>
</segment>
</net>
<net name="FSR1">
<segment>
<pinref part="MICRO" gate="1" pin="PC0(ADC0/PCINT8)"/>
</segment>
<segment>
<pinref part="R-FSR1" gate="G$1" pin="1"/>
<pinref part="FSR-1" gate="-1" pin="KL"/>
</segment>
</net>
<net name="FSR2">
<segment>
<pinref part="MICRO" gate="1" pin="PC1(ADC1/PCINT9)"/>
</segment>
<segment>
<pinref part="R-FSR2" gate="G$1" pin="1"/>
<pinref part="FSR-2" gate="-1" pin="KL"/>
</segment>
</net>
<net name="N$8">
<segment>
</segment>
</net>
<net name="MOTOR-1">
<segment>
<pinref part="MICRO" gate="1" pin="PD5(T1/OC0B/PCINT21)"/>
</segment>
<segment>
<pinref part="MOTOR1" gate="-1" pin="S"/>
</segment>
</net>
<net name="MOTOR-2">
<segment>
<pinref part="MICRO" gate="1" pin="PD6(AIN0/OC0A/PCINT22)"/>
</segment>
<segment>
<pinref part="MOTOR2" gate="-1" pin="S"/>
</segment>
</net>
<net name="N$1">
<segment>
</segment>
</net>
<net name="TX-BLUE">
<segment>
<pinref part="MICRO" gate="1" pin="PD2(INT0/PCINT18)"/>
</segment>
<segment>
<pinref part="HM-10" gate="-3" pin="S"/>
</segment>
</net>
<net name="RX-BLUE">
<segment>
<pinref part="MICRO" gate="1" pin="PD3(INT1/OC2B/PCINT19)"/>
</segment>
<segment>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$4">
<segment>
</segment>
</net>
<net name="V-LEVEL">
<segment>
<pinref part="MICRO" gate="1" pin="PC2(ADC2/PCINT10)"/>
</segment>
<segment>
<pinref part="R1-LEVEL" gate="G$1" pin="2"/>
<pinref part="R2-LEVEL" gate="G$1" pin="1"/>
<pinref part="ZENER-LEVEL" gate="G$1" pin="C"/>
</segment>
</net>
<net name="N$15">
<segment>
</segment>
</net>
<net name="INPUT+">
<segment>
<pinref part="IC1" gate="1" pin="IN"/>
<pinref part="C14" gate="G$1" pin="+"/>
<pinref part="+--GND" gate="-1" pin="KL"/>
</segment>
<segment>
<pinref part="C12" gate="G$1" pin="+"/>
<pinref part="IC2" gate="1" pin="IN"/>
</segment>
<segment>
<pinref part="R1-LEVEL" gate="G$1" pin="1"/>
</segment>
</net>
<net name="OUTPUT-12V">
<segment>
<pinref part="C13" gate="G$1" pin="+"/>
<pinref part="IC2" gate="1" pin="OUT"/>
</segment>
<segment>
<pinref part="+--R" gate="-2" pin="KL"/>
</segment>
</net>
<net name="N$16">
<segment>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="R1-LED" gate="G$1" pin="2"/>
<pinref part="R1-LED1" gate="G$1" pin="1"/>
<pinref part="MOSFET-LED1" gate="NMOS" pin="G"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="R2-LED" gate="G$1" pin="1"/>
<pinref part="R1-LED2" gate="G$1" pin="1"/>
<pinref part="MOSFET-LED2" gate="NMOS" pin="G"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="R1-LED3" gate="G$1" pin="1"/>
<pinref part="R3-LED" gate="G$1" pin="1"/>
<pinref part="MOSFET-LED3" gate="NMOS" pin="G"/>
</segment>
</net>
<net name="N$13">
<segment>
</segment>
</net>
<net name="N$14">
<segment>
</segment>
</net>
<net name="N$18">
<segment>
</segment>
</net>
<net name="N$19">
<segment>
<pinref part="MICRO" gate="1" pin="PB6(XTAL1/TOSC1/PCINT6)"/>
<pinref part="CRYSTAL" gate="G$1" pin="2"/>
<pinref part="C1" gate="A" pin="C2"/>
</segment>
</net>
<net name="N$21">
<segment>
<pinref part="MICRO" gate="1" pin="PB7(XTAL2/TOSC2/PCINT7)"/>
<pinref part="CRYSTAL" gate="G$1" pin="1"/>
<pinref part="C2" gate="A" pin="C2"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="MICRO" gate="1" pin="PB4(MISO/PCINT4)"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="6"/>
</segment>
</net>
<net name="N$2">
<segment>
</segment>
</net>
<net name="RX-FTDI">
<segment>
<pinref part="MICRO" gate="1" pin="PD0(RXD/PCINT16)"/>
</segment>
<segment>
<pinref part="FTDI" gate="A" pin="4"/>
</segment>
</net>
<net name="TX-FTDI">
<segment>
<pinref part="MICRO" gate="1" pin="PD1(TXD/PCINT17)"/>
</segment>
<segment>
<pinref part="FTDI" gate="A" pin="5"/>
</segment>
</net>
<net name="RESET-SPI">
<segment>
<pinref part="SWITCH" gate="2" pin="P"/>
<pinref part="SWITCH" gate="2" pin="P1"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="MICRO" gate="1" pin="PC6(/RESET/PCINT14)"/>
<pinref part="C6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="SPI" gate="A" pin="2"/>
</segment>
</net>
<net name="N$3">
<segment>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="R5" gate="G$1" pin="2"/>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="HM-10" gate="-4" pin="S"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
