<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="22.413878125" y1="16.84288125" x2="80.8668875" y2="16.802421875" width="0" layer="20"/>
<wire x1="80.8668875" y1="16.802421875" x2="80.808253125" y2="70.643575" width="0" layer="20"/>
<wire x1="80.808253125" y1="70.643575" x2="22.490346875" y2="70.608971875" width="0" layer="20"/>
<wire x1="22.490346875" y1="70.608971875" x2="22.413878125" y2="16.84288125" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_LONGPADS">
</package>
<package name="1X04_LONGPADS">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X01_LONGPAD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
<package name="1X03_LONGPADS">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C2" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C3" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C4" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C5" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C6" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="CONN3" library="01_SparkFun" package="1X08_LONGPADS" value=""/>
<element name="FTDI" library="SparkFun-Connectors" package="1X06-SMD" value="">
<attribute name="PROD_ID" value="CONN-08971"/>
</element>
<element name="HEADER" library="01_FAB_Hello" package="2X03SMD" value=""/>
<element name="LED" library="01_FAB_Hello" package="1206" value="green"/>
<element name="PAD1" library="wirepad" package="2,54/0,9" value=""/>
<element name="R1" library="01_FAB_Hello" package="1206" value="499"/>
<element name="R2" library="01_FAB_Hello" package="1206" value="499"/>
<element name="REGULATOR" library="01_fab" package="SOT23" value=""/>
<element name="S2" library="01_FAB_Hello" package="6MM_SWITCH" value=""/>
<element name="U$1" library="01_fab" package="EFOBM" value="RESONATOR"/>
<element name="U2" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="JP2" library="01_SparkFun" package="1X04_LONGPADS" value=""/>
<element name="JP3" library="01_SparkFun" package="1X04_LONGPADS" value=""/>
<element name="JP5" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="JP4" library="SparkFun-Connectors" package="1X03_LONGPADS" value=""/>
<element name="R4" library="01_FAB_Hello" package="1206" value="0"/>
<element name="JP6" library="01_SparkFun" package="1X01_LONGPAD" value=""/>
<element name="R3" library="01_FAB_Hello" package="1206" value="0"/>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPDT-SMD" value=""/>
<element name="JP1" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP7" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="R5" library="01_FAB_Hello" package="1206" value="0"/>
</elements>
<signals>
<signal name="XTAL1">
<contactref element="U2" pad="7"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="XTAL2">
<contactref element="U2" pad="8"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="REGULATOR" pad="3"/>
<contactref element="LED" pad="2"/>
<contactref element="HEADER" pad="6"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="U2" pad="21"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="FTDI" pad="6"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="HEADER" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="20"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="18"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="15"/>
<contactref element="CONN3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="16"/>
<contactref element="CONN3" pad="1"/>
<contactref element="HEADER" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="HEADER" pad="3"/>
<contactref element="U2" pad="17"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="RST">
<contactref element="HEADER" pad="5"/>
<contactref element="U2" pad="29"/>
<contactref element="S2" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="PAD1" pad="1"/>
<contactref element="S2" pad="4"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U2" pad="30"/>
<contactref element="FTDI" pad="2"/>
</signal>
<signal name="TX">
<contactref element="U2" pad="31"/>
<contactref element="FTDI" pad="3"/>
</signal>
<signal name="DTR">
<contactref element="C1" pad="1"/>
<contactref element="FTDI" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="FTDI" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="A0">
<contactref element="U2" pad="23"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="A1">
<contactref element="U2" pad="24"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="A2">
<contactref element="U2" pad="25"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A3">
<contactref element="U2" pad="26"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="A4">
<contactref element="U2" pad="27"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="A5">
<contactref element="U2" pad="28"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="A6">
<contactref element="U2" pad="19"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="A7">
<contactref element="U2" pad="22"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="D2">
<contactref element="U2" pad="32"/>
</signal>
<signal name="D3">
<contactref element="U2" pad="1"/>
</signal>
<signal name="D4">
<contactref element="U2" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U2" pad="9"/>
<contactref element="CONN3" pad="8"/>
</signal>
<signal name="D6">
<contactref element="U2" pad="10"/>
<contactref element="CONN3" pad="7"/>
</signal>
<signal name="D7">
<contactref element="U2" pad="11"/>
<contactref element="CONN3" pad="6"/>
</signal>
<signal name="B0">
<contactref element="U2" pad="12"/>
<contactref element="CONN3" pad="5"/>
</signal>
<signal name="B1">
<contactref element="U2" pad="13"/>
<contactref element="CONN3" pad="4"/>
</signal>
<signal name="B2">
<contactref element="U2" pad="14"/>
<contactref element="CONN3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="HEADER" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C3" pad="2"/>
<contactref element="REGULATOR" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="VCCIN-UF">
<contactref element="JP1" pad="1"/>
<contactref element="REGULATOR" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VCCIN-F">
<contactref element="FTDI" pad="4"/>
<contactref element="JP7" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
