<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="43.276546875" y1="28.884721875" x2="83.40691875" y2="28.884721875" width="0" layer="20"/>
<wire x1="83.40691875" y1="28.884721875" x2="83.40691875" y2="61.586365625" width="0" layer="20"/>
<wire x1="83.40691875" y1="61.586365625" x2="43.276546875" y2="61.586365625" width="0" layer="20"/>
<wire x1="43.276546875" y1="61.586365625" x2="43.276546875" y2="28.884721875" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LUXEON-PAD">
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_FAB_Hello" package="1206" value="0.1uF"/>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="0.1uF"/>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="0.1uF"/>
<element name="E1" library="01_SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="E2" library="01_SparkFun" package="LUXEON-PAD" value="M01SMD"/>
<element name="IC1" library="01_fab" package="SOT23" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="JP2" library="01_fab" package="2X03SMD" value=""/>
<element name="LED1" library="adafruit" package="WS2812" value="WS2812"/>
<element name="R1" library="01_FAB_Hello" package="1206" value="150"/>
<element name="R2" library="01_FAB_Hello" package="1206" value="10k"/>
<element name="U$1" library="01_ng" package="SOIC8" value="ATTINY45SI"/>
<element name="R4" library="01_FAB_Hello" package="1206" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED1" pad="VSS"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="E2" pad="P$1"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="LEDOUT">
<contactref element="LED1" pad="DO"/>
</signal>
<signal name="VDD">
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="VDD"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="LEDVDD"/>
<contactref element="U$1" pad="8"/>
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="LEDIN">
<contactref element="LED1" pad="DI"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="ELECTRODE">
<contactref element="E1" pad="P$1"/>
<contactref element="U$1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="7"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
