<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="30" width="0" layer="20"/>
<wire x1="100" y1="30" x2="0" y2="30" width="0" layer="20"/>
<wire x1="0" y1="30" x2="0" y2="0" width="0" layer="20"/>
<text>LED ARRAY_Prototype 2</text>
<text>Board 5_</text>
</plain>
<libraries>
<library name="00_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C41" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C42" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C43" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C44" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C45" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C46" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C47" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C48" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C49" library="00_SparkFun" package="EIA3528" value=""/>
<element name="C50" library="00_SparkFun" package="EIA3528" value=""/>
</elements>
<signals>
<signal name="EX_R1">
<contactref element="C47" pad="C"/>
<contactref element="C48" pad="A"/>
<contactref element="C49" pad="C"/>
<contactref element="C50" pad="A"/>
</signal>
<signal name="EX_R2">
<contactref element="C47" pad="A"/>
<contactref element="C48" pad="C"/>
<contactref element="C46" pad="A"/>
<contactref element="C45" pad="C"/>
<contactref element="C41" pad="C"/>
<contactref element="C42" pad="A"/>
</signal>
<signal name="EX_R7">
<contactref element="C41" pad="A"/>
<contactref element="C42" pad="C"/>
<contactref element="C43" pad="A"/>
<contactref element="C44" pad="C"/>
</signal>
<signal name="EX_R8">
<contactref element="C45" pad="A"/>
<contactref element="C46" pad="C"/>
<contactref element="C49" pad="A"/>
<contactref element="C50" pad="C"/>
<contactref element="C43" pad="C"/>
<contactref element="C44" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
